,A Diam##LENGTH##MILLIMETERS,B Diam##LENGTH##MILLIMETERS,G##LENGTH##MILLIMETERS,N##LENGTH##MILLIMETERS,Hub Diam##LENGTH##MILLIMETERS,Description##OTHER##,URL##OTHER##,Model##OTHER##,SeperateGVCase##OTHER##,Revision##OTHER##
APGV031050,315,380,500,300,78.75,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV031050,0,A
APGV031060,315,380,600,400,78.75,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV031060,0,A
APGV040055,400,485,550,350,100,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV040055,0,A
APGV040065,400,485,650,450,100,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV040065,0,A
APGV050055,500,585,550,350,125,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV050055,0,A
APGV050065,500,585,650,450,125,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV050065,0,A
APGV050070,500,585,700,500,125,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV050070,0,A
APGV056055,560,645,550,350,140,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV056055,0,A
APGV056065,560,645,650,450,140,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV056065,0,A
APGV056070,560,645,700,500,140,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV056070,0,A
APGV063055,630,715,550,350,157.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV063055,0,A
APGV063065,630,715,650,450,157.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV063065,0,A
APGV063070,630,715,700,500,157.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV063070,0,A
APGV071060,710,795,600,400,177.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV071060,0,A
APGV071070,710,795,700,500,177.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV071070,0,A
APGV071075,710,795,750,550,177.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV071075,0,A
APGV080060,800,885,600,400,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV080060,0,A
APGV080070,800,885,700,500,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV080070,0,A
APGV080075,800,885,750,550,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV080075,0,A
APGV080090,800,885,900,700,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV080090,0,A
APGV080110,800,885,1100,900,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV080110,0,A
APGV090070,900,1006,700,500,225,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV090070,0,A
APGV090075,900,1006,750,550,225,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV090075,0,A
APGV090090,900,1006,900,700,225,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV090090,0,A
APGV090110,900,1006,1100,900,225,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV090110,0,A
APGV100070,1000,1106,700,500,250,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV100070,0,A
APGV100075,1000,1106,750,550,250,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV100075,0,A
APGV100090,1000,1106,900,700,250,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV100090,0,A
APGV100110,1000,1106,1100,900,250,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV100110,0,A
APECGV031050,315,380,500,300,78.75,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV031050,0,A
APECGV031060,315,380,600,400,78.75,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV031060,0,A
APECGV040055,400,485,550,350,100,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV040055,0,A
APECGV040065,400,485,650,450,100,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV040065,0,A
APECGV050055,500,585,550,350,125,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV050055,0,A
APECGV050065,500,585,650,450,125,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV050065,0,A
APECGV050070,500,585,700,500,125,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV050070,0,A
APECGV056055,560,645,550,350,140,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV056055,0,A
APECGV056065,560,645,650,450,140,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV056065,0,A
APECGV056070,560,645,700,500,140,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV056070,0,A
APECGV063055,630,715,550,350,157.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV063055,0,A
APECGV063065,630,715,650,450,157.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV063065,0,A
APECGV063070,630,715,700,500,157.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV063070,0,A
APECGV071060,710,795,600,400,177.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV071060,0,A
APECGV071070,710,795,700,500,177.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV071070,0,A
APECGV071075,710,795,750,550,177.5,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV071075,0,A
APECGV080060,800,885,600,400,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV080060,0,A
APECGV080070,800,885,700,500,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV080070,0,A
APECGV080075,800,885,750,550,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV080075,0,A
APECGV080090,800,885,900,700,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV080090,0,A
APECGV080110,800,885,1100,900,200,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV080110,0,A
APECGV090070,900,1006,700,500,225,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV090070,0,A
APECGV090075,900,1006,750,550,225,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV090075,0,A
APECGV090090,900,1006,900,700,225,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV090090,0,A
APECGV090110,900,1006,1100,900,225,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV090110,0,A
APECGV100070,1000,1106,700,500,250,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV100070,0,A
APECGV100075,1000,1106,750,550,250,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV100075,0,A
APECGV100090,1000,1106,900,700,250,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV100090,0,A
APECGV100110,1000,1106,1100,900,250,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV100110,0,A
APGV125060255,1250,1356,900,600,255,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125060255,1,A
APGV125060350,1250,1356,1000,600,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125060350,1,A
APGV125060400,1250,1356,1000,600,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125060400,1,A
APGV125060550,1250,1356,1200,600,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125060550,1,A
APGV125080255,1250,1356,1100,800,255,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125080255,1,A
APGV125080350,1250,1356,1200,800,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125080350,1,A
APGV125080400,1250,1356,1200,800,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125080400,1,A
APGV125080550,1250,1356,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125080550,1,A
APGV125100350,1250,1356,1400,1000,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125100350,1,A
APGV125100400,1250,1356,1400,1000,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125100400,1,A
APGV125100550,1250,1356,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV125100550,1,A
APGV140060350,1400,1526,1000,600,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140060350,1,A
APGV140060400,1400,1526,1000,600,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140060400,1,A
APGV140060550,1400,1526,1200,600,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140060550,1,A
APGV140080350,1400,1526,1200,800,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140080350,1,A
APGV140080400,1400,1526,1200,800,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140080400,1,A
APGV140080550,1400,1526,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140080550,1,A
APGV140100350,1400,1526,1400,1000,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140100350,1,A
APGV140100400,1400,1526,1400,1000,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140100400,1,A
APGV140100550,1400,1526,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140100550,1,A
APGV140120400,1400,1526,1600,1200,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140120400,1,A
APGV140120550,1400,1526,1800,1200,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140120550,1,A
APGV140150400,1400,1526,1900,1500,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140150400,1,A
APGV140150550,1400,1526,2100,1500,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV140150550,1,A
APGV160080400,1600,1730,1200,800,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV160080400,1,A
APGV160080550,1600,1730,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV160080550,1,A
APGV160100400,1600,1730,1400,1000,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV160100400,1,A
APGV160100550,1600,1730,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV160100550,1,A
APGV160120400,1600,1730,1600,1200,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV160120400,1,A
APGV160120550,1600,1730,1800,1200,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV160120550,1,A
APGV160150400,1600,1730,1900,1500,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV160150400,1,A
APGV160150550,1600,1730,2100,1500,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV160150550,1,A
APGV180080550,1800,1960,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV180080550,1,A
APGV180100550,1800,1960,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV180100550,1,A
APGV180120550,1800,1960,1800,1200,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV180120550,1,A
APGV180150550,1800,1960,2100,1500,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV180150550,1,A
APGV200080550,2000,2160,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV200080550,1,A
APGV200100550,2000,2160,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV200100550,1,A
APGV200120550,2000,2160,1800,1200,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV200120550,1,A
APGV200150550,2000,2160,2100,1500,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APGV200150550,1,A
APECGV125060255,1250,1356,900,600,255,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125060255,1,A
APECGV125060350,1250,1356,1000,600,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125060350,1,A
APECGV125060400,1250,1356,1000,600,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125060400,1,A
APECGV125060550,1250,1356,1200,600,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125060550,1,A
APECGV125080255,1250,1356,1100,800,255,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125080255,1,A
APECGV125080350,1250,1356,1200,800,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125080350,1,A
APECGV125080400,1250,1356,1200,800,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125080400,1,A
APECGV125080550,1250,1356,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125080550,1,A
APECGV125100350,1250,1356,1400,1000,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125100350,1,A
APECGV125100400,1250,1356,1400,1000,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125100400,1,A
APECGV125100550,1250,1356,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV125100550,1,A
APECGV140060350,1400,1526,1000,600,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140060350,1,A
APECGV140060400,1400,1526,1000,600,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140060400,1,A
APECGV140060550,1400,1526,1200,600,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140060550,1,A
APECGV140080350,1400,1526,1200,800,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140080350,1,A
APECGV140080400,1400,1526,1200,800,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140080400,1,A
APECGV140080550,1400,1526,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140080550,1,A
APECGV140100350,1400,1526,1400,1000,350,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140100350,1,A
APECGV140100400,1400,1526,1400,1000,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140100400,1,A
APECGV140100550,1400,1526,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140100550,1,A
APECGV140120400,1400,1526,1600,1200,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140120400,1,A
APECGV140120550,1400,1526,1800,1200,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140120550,1,A
APECGV140150400,1400,1526,1900,1500,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140150400,1,A
APECGV140150550,1400,1526,2100,1500,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV140150550,1,A
APECGV160080400,1600,1730,1200,800,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV160080400,1,A
APECGV160080550,1600,1730,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV160080550,1,A
APECGV160100400,1600,1730,1400,1000,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV160100400,1,A
APECGV160100550,1600,1730,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV160100550,1,A
APECGV160120400,1600,1730,1600,1200,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV160120400,1,A
APECGV160120550,1600,1730,1800,1200,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV160120550,1,A
APECGV160150400,1600,1730,1900,1500,400,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV160150400,1,A
APECGV160150550,1600,1730,2100,1500,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV160150550,1,A
APECGV180080550,1800,1960,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV180080550,1,A
APECGV180100550,1800,1960,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV180100550,1,A
APECGV180120550,1800,1960,1800,1200,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV180120550,1,A
APECGV180150550,1800,1960,2100,1500,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV180150550,1,A
APECGV200080550,2000,2160,1400,800,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV200080550,1,A
APECGV200100550,2000,2160,1600,1000,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV200100550,1,A
APECGV200120550,2000,2160,1800,1200,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV200120550,1,A
APECGV200150550,2000,2160,2100,1500,550,"The addition of downstream guide vanes to a suitable AP range, greatly improves fan efficiency by generating more static pressure with no additional power consumption.",https://www.fantech.com.au/FanRange.aspx?AppID=I4&RangeID=1611,APECGV200150550,1,A
