,dB(A) @ 3m##OTHER##,calc_e##LENGTH##MILLIMETERS,calc_d##LENGTH##MILLIMETERS,calc_a##LENGTH##MILLIMETERS,ZoneServed##OTHER##,WireGuardInstalled##OTHER##,WarrantyDurationMonths##OTHER##,URL##OTHER##,TotalMass##MASS##KILOGRAMS,TotalEfficiency##HVAC_FACTOR##PERCENTAGE,Tile Roof Flashing##OTHER##,SystemServed##OTHER##,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyPhase##OTHER##,SupplyFrequency##ELECTRICAL_FREQUENCY##HERTZ,SpringStaticDeflectionMin##LENGTH##MILLIMETERS,SoundPressureat3m##OTHER##,SerialNumber##OTHER##,RunLoadAmps##ELECTRICAL_CURRENT##AMPERES,RFID##OTHER##,ProductCode##OTHER##,Pressure Drop - Total##HVAC_PRESSURE##PASCALS,Pressure Drop - Static##HVAC_PRESSURE##PASCALS,PrecommissioningInspectionTestPlan##OTHER##,PowerSource##OTHER##,PowerFactorState##OTHER##,PowerFactor##OTHER##,PeakPower##ELECTRICAL_POWER##WATTS,OverloadSettingActual##ELECTRICAL_CURRENT##AMPERES,OutletPWL8kHz##OTHER##,OutletPWL63Hz##OTHER##,OutletPWL500Hz##OTHER##,OutletPWL4kHz##OTHER##,OutletPWL2kHz##OTHER##,OutletPWL250Hz##OTHER##,OutletPWL1kHz##OTHER##,OutletPWL125Hz##OTHER##,OutletConeFitted##OTHER##,Outlet Velocity##HVAC_VELOCITY##METERS_PER_SECOND,OperatingTempMax##HVAC_TEMPERATURE##CELSIUS,OperatingMaintenanceManual##OTHER##,NCC_SEC_J_Compliance##OTHER##,NCC_Classification##OTHER##,NATspecWorkSection##OTHER##,MountingType##OTHER##,MountingFeetInstalled##OTHER##,MountingArrangement##OTHER##,MotorWindingInsulation##OTHER##,MotorVoltageActual##ELECTRICAL_POTENTIAL##VOLTS,MotorType##OTHER##,MotorTropicProofing##OTHER##,MotorThermistorFitted##OTHER##,MotorStarterSpeedControlType##OTHER##,MotorSize##ELECTRICAL_POWER##WATTS,MotorPoles##OTHER##,MotorManufacturer##OTHER##,MotorIngressProtectionRating##OTHER##,MotorFrame##OTHER##,MotorEfficiencyClass##OTHER##,MotorAmpsActual##ELECTRICAL_CURRENT##AMPERES,MotorAbsorbedPowerActual##ELECTRICAL_POWER##WATTS,Motor Input Power##ELECTRICAL_POWER##WATTS,Model##OTHER##,Metal deck flashing##OTHER##,MediumType##OTHER##,MediumDensity##HVAC_DENSITY##KILOGRAMS_PER_CUBIC_METER,Manufacturer##OTHER##,MaintenanceType##OTHER##,Low Speed Start Current##ELECTRICAL_POWER##WATTS,Low Speed Full Load Current##ELECTRICAL_POWER##WATTS,Location##OTHER##,LoadSubClassificationMotor##OTHER##,LoadClassification##OTHER##,Installer##OTHER##,InstallationDate##OTHER##,InletStaticPressureActual##HVAC_PRESSURE##PASCALS,InletPWL8kHz##OTHER##,InletPWL63Hz##OTHER##,InletPWL500Hz##OTHER##,InletPWL4kHz##OTHER##,InletPWL2kHz##OTHER##,InletPWL250Hz##OTHER##,InletPWL1kHz##OTHER##,InletPWL125Hz##OTHER##,InletConeInstalled##OTHER##,ImpellerBladePitch##ANGLE##DEGREES,ImpellerBladeMaterial##OTHER##,Impeller Style##OTHER##,Impeller Limit Load Power##ELECTRICAL_POWER##WATTS,Impeller Diameter##LENGTH##MILLIMETERS,Impeller Absorbed  Power##ELECTRICAL_POWER##WATTS,HazardClassification##OTHER##,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,Finish##OTHER##,FanType##OTHER##,FanStaticDutyPressure##HVAC_PRESSURE##PASCALS,FanStandard##OTHER##,FanRotationSpeedMax##OTHER##,FanRotationSpeedDesign##OTHER##,FanRotationSpeedActual##OTHER##,FanMEP##OTHER##,FanImpellerNoOfBlades##OTHER##,FanHubDiameter##LENGTH##MILLIMETERS,FanDiscInductPWL_Outlet##OTHER##,FanDiscInductPWL_Inlet##OTHER##,FanDesignArrangement##OTHER##,FanApplication##OTHER##,FanAirFlowDesign##HVAC_AIR_FLOW##LITERS_PER_SECOND,FanAirFlowCalculated##HVAC_AIR_FLOW##LITERS_PER_SECOND,FanAirFlowActual##HVAC_AIR_FLOW##LITERS_PER_SECOND,EØ##LENGTH##MILLIMETERS,ExpectedServiceLifeYears##OTHER##,EnergyMeterGrouping##OTHER##,DØ##LENGTH##MILLIMETERS,DynamicPressureActual##HVAC_PRESSURE##PASCALS,DuctSystemStaticPressureCalculated##HVAC_PRESSURE##PASCALS,DischargeStaticPressureActual##HVAC_PRESSURE##PASCALS,DimensionalTolerance##LENGTH##MILLIMETERS,Designer##OTHER##,Description##OTHER##,ComponentStatus##OTHER##,ComponentName##OTHER##,CommissioningTechnician##OTHER##,CommissioningDate##OTHER##,Client##OTHER##,C##LENGTH##MILLIMETERS,BasisOfDesign##OTHER##,Barcode##OTHER##,B##LENGTH##MILLIMETERS,AØ##LENGTH##MILLIMETERS,AssetIdentifier##OTHER##,Approx Volume##VOLUME##CUBIC_METERS,AirFlowMin##HVAC_AIR_FLOW##LITERS_PER_SECOND,AirFlowMax##HVAC_AIR_FLOW##LITERS_PER_SECOND,AirFlowDesign##HVAC_AIR_FLOW##LITERS_PER_SECOND,AirFlowCalc##HVAC_AIR_FLOW##LITERS_PER_SECOND,AirFlowActual##HVAC_AIR_FLOW##LITERS_PER_SECOND,AirFlow##HVAC_AIR_FLOW##LITERS_PER_SECOND,AbsorbedPower##ELECTRICAL_POWER##WATTS
ECE152SM,0,75,222.5,70,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/thruroofsupply.pdf,0,0,0,,0,1,0,0,0,,0,,,0,0,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,ECE152MS,0,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,0,<By Category>,,0,,0,0,0,,,0,0,0,,,0,0,0,150,0,,445,0,0,0,0,,The Ezifit Thru Roof supply air fan provides fresh filtered air to internal spaces and is suitable for tile or metal deck type roofs. It includes a high performance fan that makes it suitable for long duct runs and a multiple number of supply points. It produces low noise within the occupied space because the fan is mounted outside the building.,,,,,,949,,,154,140,,0,0,0,0,0,0,0,0
ECE152ST,0,75,222.5,70,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/thruroofsupply.pdf,0,0,0,,0,1,0,0,0,,0,,,0,0,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,ECE152TS,0,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,0,<By Category>,,0,,0,0,0,,,0,0,0,,,0,0,0,150,0,,445,0,0,0,0,,The Ezifit Thru Roof supply air fan provides fresh filtered air to internal spaces and is suitable for tile or metal deck type roofs. It includes a high performance fan that makes it suitable for long duct runs and a multiple number of supply points. It produces low noise within the occupied space because the fan is mounted outside the building.,,,,,,949,,,154,140,,0,0,0,0,0,0,0,0
