,y1##LENGTH##MILLIMETERS,x1##LENGTH##MILLIMETERS,TotalMass##MASS##KILOGRAMS,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyPhase##OTHER##,Size OA##LENGTH##MILLIMETERS,Opening Size##LENGTH##MILLIMETERS,Model##OTHER##,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanRotationSpeedDesign##OTHER##,FanAirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,D##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,Base OA##LENGTH##MILLIMETERS,Approx Volume##VOLUME##CUBIC_METERS,AbsorbedPower##ELECTRICAL_POWER##VOLT_AMPERES
CEEC31VGL,310,520,0,0,1,520,310,CEEC31VGL,0,0,0,310,50,410,0,0
CEEC35VGL,400,670,0,0,1,670,400,CEEC35VGL,0,0,0,400,50,500,0,0
CEEC45VGL,525,900,0,0,1,900,620,CEEC45VGL,0,0,0,525,50,720,0,0
CDEC63VGL,710,1160,0,0,1,1160,710,CDEC63VGL,0,0,0,710,50,810,0,0
