,dB(A) @ 3m##OTHER##,ZoneServed##OTHER##,WireGuardInstalled##OTHER##,WarrantyDurationMonths##OTHER##,URL##OTHER##,Type Comments##OTHER##,TotalMass##MASS##KILOGRAMS,TotalEfficiency##HVAC_FACTOR##PERCENTAGE,SystemServed##OTHER##,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyPhase##OTHER##,SupplyFrequency##ELECTRICAL_FREQUENCY##HERTZ,SpringStaticDeflectionMin##LENGTH##MILLIMETERS,SoundPressureat3m##OTHER##,SerialNumber##OTHER##,RunLoadAmps##ELECTRICAL_CURRENT##AMPERES,RFID##OTHER##,ProductCode##OTHER##,PrecommissioningInspectionTestPlan##OTHER##,PowerSource##OTHER##,PowerFactorState##OTHER##,PowerFactor##OTHER##,PeakPower##ELECTRICAL_POWER##VOLT_AMPERES,OverloadSettingActual##ELECTRICAL_CURRENT##AMPERES,OutletPWL8kHz##OTHER##,OutletPWL63Hz##OTHER##,OutletPWL500Hz##OTHER##,OutletPWL4kHz##OTHER##,OutletPWL2kHz##OTHER##,OutletPWL250Hz##OTHER##,OutletPWL1kHz##OTHER##,OutletPWL125Hz##OTHER##,OutletConeFitted##OTHER##,OperatingTempMax##HVAC_TEMPERATURE##CELSIUS,OperatingMaintenanceManual##OTHER##,NCC_SEC_J_Compliance##OTHER##,NCC_Classification##OTHER##,NATspecWorkSection##OTHER##,MountingType##OTHER##,MountingFeetInstalled##OTHER##,MountingArrangement##OTHER##,MotorWindingInsulation##OTHER##,MotorVoltageActual##ELECTRICAL_POTENTIAL##VOLTS,MotorType##OTHER##,MotorTropicProofing##OTHER##,MotorThermistorFitted##OTHER##,MotorStarterSpeedControlType##OTHER##,MotorSize##ELECTRICAL_POWER##VOLT_AMPERES,MotorPoles##OTHER##,MotorManufacturer##OTHER##,MotorIngressProtectionRating##OTHER##,MotorFrame##OTHER##,MotorEfficiencyClass##OTHER##,MotorAmpsActual##ELECTRICAL_CURRENT##AMPERES,MotorAbsorbedPowerActual##ELECTRICAL_POWER##VOLT_AMPERES,MediumType##OTHER##,MediumDensity##HVAC_DENSITY##POUNDS_MASS_PER_CUBIC_FOOT,MaintenanceType##OTHER##,Location##OTHER##,LoadSubClassificationMotor##OTHER##,LoadClassification##OTHER##,Installer##OTHER##,InstallationDate##OTHER##,InletStaticPressureActual##HVAC_PRESSURE##PASCALS,InletPWL8kHz##OTHER##,InletPWL63Hz##OTHER##,InletPWL500Hz##OTHER##,InletPWL4kHz##OTHER##,InletPWL2kHz##OTHER##,InletPWL250Hz##OTHER##,InletPWL1kHz##OTHER##,InletPWL125Hz##OTHER##,InletConeInstalled##OTHER##,ImpellerBladePitch##ANGLE##DEGREES,ImpellerBladeMaterial##OTHER##,HazardClassification##OTHER##,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanType##OTHER##,FanStaticDutyPressure##HVAC_PRESSURE##PASCALS,FanStandard##OTHER##,FanRotationSpeedMax##OTHER##,FanRotationSpeedDesign##OTHER##,FanRotationSpeedActual##OTHER##,FanMEP##OTHER##,FanImpellerNoOfBlades##OTHER##,FanHubDiameter##LENGTH##MILLIMETERS,FanDiscInductPWL_Outlet##OTHER##,FanDiscInductPWL_Inlet##OTHER##,FanDesignArrangement##OTHER##,FanApplication##OTHER##,FanAirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowCalculated##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,F##LENGTH##MILLIMETERS,ExpectedServiceLifeYears##OTHER##,EnergyMeterGrouping##OTHER##,Pressure Drop - Total##HVAC_PRESSURE##PASCALS,Pressure Drop - Static##HVAC_PRESSURE##PASCALS,Outlet Velocity##HVAC_VELOCITY##FEET_PER_MINUTE,Motor Input Power##ELECTRICAL_POWER##VOLT_AMPERES,Model##OTHER##,Manufacturer##OTHER##,Low Speed Start Current##ELECTRICAL_POWER##VOLT_AMPERES,Low Speed Full Load Current##ELECTRICAL_POWER##VOLT_AMPERES,E##LENGTH##MILLIMETERS,DynamicPressureActual##HVAC_PRESSURE##PASCALS,DuctSystemStaticPressureCalculated##HVAC_PRESSURE##PASCALS,DischargeStaticPressureActual##HVAC_PRESSURE##PASCALS,DimensionalTolerance##LENGTH##MILLIMETERS,Designer##OTHER##,D##LENGTH##MILLIMETERS,ComponentStatus##OTHER##,ComponentName##OTHER##,CommissioningTechnician##OTHER##,CommissioningDate##OTHER##,Client##OTHER##,CRadius##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,BasisOfDesign##OTHER##,Barcode##OTHER##,B##LENGTH##MILLIMETERS,AssetIdentifier##OTHER##,AirFlowMin##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowMax##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowCalc##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlow##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AbsorbedPower##ELECTRICAL_POWER##VOLT_AMPERES,Impeller Style##OTHER##,Impeller Limit Load Power##ELECTRICAL_POWER##VOLT_AMPERES,Impeller Diameter##LENGTH##MILLIMETERS,Impeller Absorbed  Power##ELECTRICAL_POWER##VOLT_AMPERES,Fan Material##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Approx Volume##VOLUME##CUBIC_METERS,Additional Notes##OTHER##,A##LENGTH##MILLIMETERS
SILDES100CZ3C-W,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,45,0,,0,0,0,0,SILDES100CZ3CW,Fantech,0,0,79,0,0,0,0,,85,,,,,,49.5,99,,,130,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,188
SILDES200CZ3C-W,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,56,0,,0,0,0,0,SILDES200CZ3CW,Fantech,0,0,80,0,0,0,0,,89,,,,,,58,116,,,145,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,210
SILDES300CZ3C-W,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,67,0,,0,0,0,0,SILDES300CZ3CW,Fantech,0,0,95,0,0,0,0,,112,,,,,,73,146,,,179,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,247
SILDES100CZ3C-S,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,45,0,,0,0,0,0,SILDES100CZ3CS,Fantech,0,0,79,0,0,0,0,,85,,,,,,49.5,99,,,130,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,188
SILDES200CZ3C-S,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,56,0,,0,0,0,0,SILDES200CZ3CS,Fantech,0,0,80,0,0,0,0,,89,,,,,,58,116,,,145,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,210
SILDES300CZ3C-S,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,67,0,,0,0,0,0,SILDES300CZ3CS,Fantech,0,0,95,0,0,0,0,,112,,,,,,73,146,,,179,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,247
SILDES100CRZ3C-W,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,45,0,,0,0,0,0,SILDES100CRZ3CW,Fantech,0,0,79,0,0,0,0,,85,,,,,,49.5,99,,,130,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,188
SILDES200CRZ3C-W,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,56,0,,0,0,0,0,SILDES200CRZ3CW,Fantech,0,0,80,0,0,0,0,,89,,,,,,58,116,,,145,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,210
SILDES300CRZ3C-W,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,67,0,,0,0,0,0,SILDES300CRZ3CW,Fantech,0,0,95,0,0,0,0,,112,,,,,,73,146,,,179,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,247
SILDES100CRZ3C-S,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,45,0,,0,0,0,0,SILDES100CRZ3CS,Fantech,0,0,79,0,0,0,0,,85,,,,,,49.5,99,,,130,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,188
SILDES200CRZ3C-S,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,56,0,,0,0,0,0,SILDES200CRZ3CS,Fantech,0,0,80,0,0,0,0,,89,,,,,,58,116,,,145,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,210
SILDES300CRZ3C-S,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,67,0,,0,0,0,0,SILDES300CRZ3CS,Fantech,0,0,95,0,0,0,0,,112,,,,,,73,146,,,179,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,247
SILDES100CHZ3C-W,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,45,0,,0,0,0,0,SILDES100CHZ3CW,Fantech,0,0,79,0,0,0,0,,85,,,,,,49.5,99,,,130,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,188
SILDES200CHZ3C-W,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,56,0,,0,0,0,0,SILDES200CHZ3CW,Fantech,0,0,80,0,0,0,0,,89,,,,,,58,116,,,145,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,210
SILDES300CHZ3C-W,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,67,0,,0,0,0,0,SILDES300CHZ3CW,Fantech,0,0,95,0,0,0,0,,112,,,,,,73,146,,,179,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,247
SILDES100CHZ3C-S,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,45,0,,0,0,0,0,SILDES100CHZ3CS,Fantech,0,0,79,0,0,0,0,,85,,,,,,49.5,99,,,130,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,188
SILDES200CHZ3C-S,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,56,0,,0,0,0,0,SILDES200CHZ3CS,Fantech,0,0,80,0,0,0,0,,89,,,,,,58,116,,,145,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,210
SILDES300CHZ3C-S,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silentdes.pdf,,0,0,,0,1,0,0,0,,0,,,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,,0,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,,0,,0,0,0,,,0,0,0,,,0,0,0,67,0,,0,0,0,0,SILDES300CHZ3CS,Fantech,0,0,95,0,0,0,0,,112,,,,,,73,146,,,179,,0,0,0,0,0,0,0,,0,0,0,Default,The Silent Design Series exhaust fans bring style and elegance to any contemporary bathroom ensuite and toilet. They can be wall or ceiling mounted and feature an advanced vibration absorbing design that ensures quiet operation. Sizes to fit 100. 125 and 150mm duct are available and models with a run-on-timer and humidistat are included in the range.,1219.2,0,,247
