,calc_c##LENGTH##MILLIMETERS,calc_a##LENGTH##MILLIMETERS,TotalMass##MASS##KILOGRAMS,Model##OTHER##,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanRotationSpeedDesign##OTHER##,FanAirFlowActual##HVAC_AIR_FLOW##LITERS_PER_SECOND,Description##OTHER##,D##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,Approx Volume##VOLUME##CUBIC_METERS,AbsorbedPower##ELECTRICAL_POWER##WATTS,A##LENGTH##MILLIMETERS
EDM-100S,49,125,0,EDM-100S,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",55,98,98,0,0,155
EDM-200S,59.5,157,0,EDM-200S,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",62,119,109,0,0,187
EDM-300S,75,170,0,EDM-300S,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",104,150,129,0,0,200
EDM-100C,49,125,0,EDM-100C,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",55,98,98,0,0,155
EDM-200C,59.5,157,0,EDM-200C,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",62,119,109,0,0,187
EDM-300C,75,170,0,EDM-300C,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",104,150,129,0,0,200
EDM-100CT,49,125,0,EDM-100CT,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",55,98,98,0,0,155
EDM-200CT,59.5,157,0,EDM-200CT,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",62,119,109,0,0,187
EDM-300CR,75,170,0,EDM-300CR,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",104,150,129,0,0,200
EDM-100S-12V,49,125,0,EDM-100S-12V,0,0,0,"The EDM Series can be wall or ceiling mounted and is designed to exhaust stale and moist air from bathrooms, toilets, laundries etc. They are also suitable for ventilating all types of small or closed areas.",55,98,98,0,0,155