,Y1##LENGTH##MILLIMETERS,X2##LENGTH##MILLIMETERS,X1##LENGTH##MILLIMETERS,Wall thinkness allowed##LENGTH##MILLIMETERS,calc_d##LENGTH##MILLIMETERS,Wall thickness##LENGTH##MILLIMETERS,TotalMass##MASS##KILOGRAMS,PowerFactor##OTHER##,Model##OTHER##,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanRotationSpeedDesign##OTHER##,FanAirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,DØ##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,AbsorbedPower##ELECTRICAL_POWER##WATTS,A##LENGTH##MILLIMETERS
HV-150AE,134,230,251,25,92.5,25,0,0,HV-150,0,0,0,185,109,251,0,230
HV-230AE,167,300,325,25,129.5,6,0,0,HV-230,0,0,0,259,142,325,0,300
HV-300AE,175,368,403,25,163.5,25,0,0,HV-300,0,0,0,327,150,403,0,368
