,A##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,D##LENGTH##MILLIMETERS,E##LENGTH##MILLIMETERS,F##LENGTH##MILLIMETERS,Description##OTHER##,URL##OTHER##,Model##OTHER##,NCC_SEC_J_Compliance##OTHER##,TotalMass##MASS##KILOGRAMS,ProtrudingSpigot##OTHER##,Revision##OTHER##
AD314S,400,500,95,380,670,10,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD314S,0,10,1,B
AD354S,400,500,95,380,670,10,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD354S,0,12,1,B
AD404S,510,610,90,450,770,25,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD404S,1,16,1,B
AD406S,510,610,90,450,770,25,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD406S,1,16,1,B
AD454S,510,610,90,450,770,25,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD454S,1,18,1,B
AD456S,510,610,90,450,770,25,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD456S,1,18,1,B
AD504S,670,770,90,560,890,30,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD504S,1,28,1,B
AD506S,670,770,90,560,890,30,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD506S,1,28,1,B
AD564S,670,770,90,560,890,30,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD564S,1,34,1,B
AD566S,670,770,90,560,890,30,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD566S,1,34,1,B
AD636S,780,980,85,640,1180,45,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AD636S,1,50,1,B
AE314S,400,500,95,380,670,10,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE314S,0,10,1,B
AE354S,400,500,95,380,670,10,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE354S,0,12,1,B
AE404S,510,610,90,450,770,25,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE404S,1,16,1,B
AE406S,510,610,90,450,770,25,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE406S,1,16,1,B
AE454S,510,610,90,450,770,25,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE454S,1,18,1,B
AE456S,510,610,90,450,770,25,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE456S,1,18,1,B
AE504S,670,770,90,560,890,30,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE504S,1,28,1,B
AE506S,670,770,90,560,890,30,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE506S,1,28,1,B
AE564S,670,770,90,560,890,30,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE564S,1,34,1,B
AE566S,670,770,90,560,890,30,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE566S,1,34,1,B
AE636S,780,980,85,640,1180,45,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,AE636S,1,50,1,B
MV112S,210,260,55,200,306,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV112S,0,2,0,A
MV132S,210,260,55,200,306,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV132S,0,2,0,A
MV202S,350,410,55,350,570,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV202S,1,5,0,B
MV204S,350,410,55,350,570,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV204S,1,5,0,B
MV252S,350,410,55,350,570,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV252S,1,6,0,B
MV254S,350,410,55,350,570,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV254S,1,7,0,B
MV302S,350,410,55,350,570,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV302S,1,7,0,B
MV304S,350,410,55,350,570,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV304S,1,7,0,B
MV306S,350,410,55,350,570,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV306S,1,7,0,B
MV354S,400,500,95,380,670,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV354S,1,9,0,B
MV356S,400,500,95,380,670,0,These robust but lightweight units from Fantech are fitted with bird mesh as standard to prevent debris and birds entering the building and interrupting motor operation.,https://www.fantech.com.au/FanRange.aspx?RangeID=39&mountingID=,MV356S,1,9,0,B
