,SupplyPhase##OTHER##,A##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,D##LENGTH##MILLIMETERS,E##LENGTH##MILLIMETERS,F##LENGTH##MILLIMETERS,G##LENGTH##MILLIMETERS,H##LENGTH##MILLIMETERS,J##LENGTH##MILLIMETERS,K##LENGTH##MILLIMETERS,Description##OTHER##,TotalMass##MASS##KILOGRAMS,Approx Volume##VOLUME##CUBIC_METERS,calc_k##LENGTH##MILLIMETERS,calc_c##LENGTH##MILLIMETERS,calc_b##LENGTH##MILLIMETERS,calc_a##LENGTH##MILLIMETERS,ZoneServed##OTHER##,Y1##LENGTH##MILLIMETERS,X1##LENGTH##MILLIMETERS,WireGuardInstalled##OTHER##,fan_guard_thick##LENGTH##MILLIMETERS,WarrantyDurationMonths##OTHER##,URL##OTHER##,Type Comments##OTHER##,TotalEfficiency##HVAC_FACTOR##PERCENTAGE,SystemServed##OTHER##,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyFrequency##ELECTRICAL_FREQUENCY##HERTZ,SpringStaticDeflectionMin##LENGTH##MILLIMETERS,SerialNumber##OTHER##,RunLoadAmps##ELECTRICAL_CURRENT##AMPERES,RFID##OTHER##,ProductCode##OTHER##,Pressure Drop - Total##HVAC_PRESSURE##PASCALS,Pressure Drop - Static##HVAC_PRESSURE##PASCALS,PrecommissioningInspectionTestPlan##OTHER##,PowerSource##OTHER##,PowerFactorState##OTHER##,PowerFactor##OTHER##,PeakPower##ELECTRICAL_POWER##WATTS,OverloadSettingActual##ELECTRICAL_CURRENT##AMPERES,OutletPWL8kHz##OTHER##,OutletPWL63Hz##OTHER##,OutletPWL500Hz##OTHER##,OutletPWL4kHz##OTHER##,OutletPWL2kHz##OTHER##,OutletPWL250Hz##OTHER##,OutletPWL1kHz##OTHER##,OutletPWL125Hz##OTHER##,OutletConeFitted##OTHER##,Outlet Velocity##HVAC_VELOCITY##METERS_PER_SECOND,OperatingTempMax##HVAC_TEMPERATURE##CELSIUS,OperatingMaintenanceManual##OTHER##,NCC_SEC_J_Compliance##OTHER##,NCC_Classification##OTHER##,NATspecWorkSection##OTHER##,MountingType##OTHER##,MountingFeetInstalled##OTHER##,MountingArrangement##OTHER##,MotorWindingInsulation##OTHER##,MotorVoltageActual##ELECTRICAL_POTENTIAL##VOLTS,MotorType##OTHER##,MotorTropicProofing##OTHER##,MotorThermistorFitted##OTHER##,MotorStarterSpeedControlType##OTHER##,MotorSize##ELECTRICAL_POWER##WATTS,MotorPoles##OTHER##,MotorManufacturer##OTHER##,MotorIngressProtectionRating##OTHER##,MotorFrame##OTHER##,MotorEfficiencyClass##OTHER##,MotorAmpsActual##ELECTRICAL_CURRENT##AMPERES,MotorAbsorbedPowerActual##ELECTRICAL_POWER##WATTS,Motor Input Power##ELECTRICAL_POWER##WATTS,Model##OTHER##,MediumType##OTHER##,MediumDensity##HVAC_DENSITY##KILOGRAMS_PER_CUBIC_METER,Material##OTHER##,Manufacturer##OTHER##,MaintenanceType##OTHER##,Low Speed Start Current##ELECTRICAL_POWER##WATTS,Low Speed Full Load Current##ELECTRICAL_POWER##WATTS,Location##OTHER##,LoadSubClassificationMotor##OTHER##,LoadClassification##OTHER##,Installer##OTHER##,InstallationDate##OTHER##,InletStaticPressureActual##HVAC_PRESSURE##PASCALS,InletPWL8kHz##OTHER##,InletPWL63Hz##OTHER##,InletPWL500Hz##OTHER##,InletPWL4kHz##OTHER##,InletPWL2kHz##OTHER##,InletPWL250Hz##OTHER##,InletPWL1kHz##OTHER##,InletPWL125Hz##OTHER##,InletConeInstalled##OTHER##,ImpellerBladePitch##ANGLE##DEGREES,ImpellerBladeMaterial##OTHER##,Impeller Style##OTHER##,Impeller Limit Load Power##ELECTRICAL_POWER##WATTS,Impeller Diameter##LENGTH##MILLIMETERS,Impeller Absorbed  Power##ELECTRICAL_POWER##WATTS,HazardClassification##OTHER##,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanType##OTHER##,FanStaticDutyPressure##HVAC_PRESSURE##PASCALS,FanStandard##OTHER##,FanRotationSpeedMax##OTHER##,FanRotationSpeedDesign##OTHER##,FanRotationSpeedActual##OTHER##,FanMEP##OTHER##,FanImpellerNoOfBlades##OTHER##,FanHubDiameter##LENGTH##MILLIMETERS,FanDiscInductPWL_Outlet##OTHER##,FanDiscInductPWL_Inlet##OTHER##,FanDesignArrangement##OTHER##,FanApplication##OTHER##,FanAirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowCalculated##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,ExpectedServiceLifeYears##OTHER##,EnergyMeterGrouping##OTHER##,DynamicPressureActual##HVAC_PRESSURE##PASCALS,DuctSystemStaticPressureCalculated##HVAC_PRESSURE##PASCALS,DischargeStaticPressureActual##HVAC_PRESSURE##PASCALS,DimensionalTolerance##LENGTH##MILLIMETERS,Designer##OTHER##,ComponentStatus##OTHER##,ComponentName##OTHER##,CommissioningTechnician##OTHER##,CommissioningDate##OTHER##,Client##OTHER##,BasisOfDesign##OTHER##,Barcode##OTHER##,AssetIdentifier##OTHER##,AirFlowMin##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowMax##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowCalc##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlow##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AbsorbedPower##ELECTRICAL_POWER##WATTS
CPEEC25,1,254,257,276,370,320,43,48,6,24,7,The Compact 2000 EC Series of square plate axial fans incorporates the latest state of the art EC motor technology. They are a high quality product suitable for a wide range of applications.,4.5,0.03,3.5,138,128.5,127,0,91,320,1,5,0,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,"D = Three phase, E = Single phase.",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,-273.15,0,1,0,0,"Wall,Window&Ceiling Mounted Type",1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,CPEEC25,0,0,<By Category>,Fantech,0,0,0,0,1,HVAC,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
CPEEC40,1,400,412,450,540,490,56,95,15,1,10,The Compact 2000 EC Series of square plate axial fans incorporates the latest state of the art EC motor technology. They are a high quality product suitable for a wide range of applications.,9.5,0.07,3.5,138,128.5,127,0,91,320,1,5,0,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,"D = Three phase, E = Single phase.",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,-273.15,0,1,0,0,"Wall,Window&Ceiling Mounted Type",1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,CPEEC40,0,0,<By Category>,Fantech,0,0,0,0,1,HVAC,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
CPEEC50,1,540,517,584,655,615,63,104,16,37,11,The Compact 2000 EC Series of square plate axial fans incorporates the latest state of the art EC motor technology. They are a high quality product suitable for a wide range of applications.,21,0.13,3.5,138,128.5,127,0,91,320,1,5,0,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,"D = Three phase, E = Single phase.",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,-273.15,0,1,0,0,"Wall,Window&Ceiling Mounted Type",1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,CPEEC50,0,0,<By Category>,Fantech,0,0,0,0,1,HVAC,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
CPDEC63,3,635,648,728,805,750,80,130,20,53,11,The Compact 2000 EC Series of square plate axial fans incorporates the latest state of the art EC motor technology. They are a high quality product suitable for a wide range of applications.,38.5,0.22,3.5,138,128.5,127,0,91,320,1,5,0,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,"D = Three phase, E = Single phase.",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,-273.15,0,1,0,0,"Wall,Window&Ceiling Mounted Type",1,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,CPDEC63,0,0,<By Category>,Fantech,0,0,0,0,1,HVAC,0,0,0,0,0,0,0,0,0,0,0,1,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0
