,dB(A) @ 3m##OTHER##,ZoneServed##OTHER##,WireGuardInstalled##OTHER##,WarrantyDurationMonths##OTHER##,URL##OTHER##,Type Comments##OTHER##,TotalMass##MASS##KILOGRAMS,TotalEfficiency##HVAC_FACTOR##PERCENTAGE,SystemServed##OTHER##,SymbolWidth##LENGTH##MILLIMETERS,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyPhase##OTHER##,SupplyFrequency##ELECTRICAL_FREQUENCY##HERTZ,SpringStaticDeflectionMin##LENGTH##MILLIMETERS,SoundPressureat3m##OTHER##,SerialNumber##OTHER##,RunLoadAmps##ELECTRICAL_CURRENT##AMPERES,RodRadius##LENGTH##MILLIMETERS,RodAlignment##LENGTH##MILLIMETERS,RFID##OTHER##,ProductCode##OTHER##,PrecommissioningInspectionTestPlan##OTHER##,PowerSource##OTHER##,PowerFactorState##OTHER##,PowerFactor##OTHER##,MountingPlateThickness##LENGTH##MILLIMETERS,MountingPlateLength##LENGTH##MILLIMETERS,PeakPower##ELECTRICAL_POWER##VOLT_AMPERES,OverloadSettingActual##ELECTRICAL_CURRENT##AMPERES,OutletPWL8kHz##OTHER##,OutletPWL63Hz##OTHER##,OutletPWL500Hz##OTHER##,OutletPWL4kHz##OTHER##,OutletPWL2kHz##OTHER##,OutletPWL250Hz##OTHER##,OutletPWL1kHz##OTHER##,OutletPWL125Hz##OTHER##,OutletConeFitted##OTHER##,OperatingTempMax##HVAC_TEMPERATURE##CELSIUS,OperatingMaintenanceManual##OTHER##,NCC_SEC_J_Compliance##OTHER##,NCC_Classification##OTHER##,NATspecWorkSection##OTHER##,MountingType##OTHER##,MountingFeetInstalled##OTHER##,MountingArrangement##OTHER##,MotorWindingInsulation##OTHER##,MotorVoltageActual##ELECTRICAL_POTENTIAL##VOLTS,MotorType##OTHER##,MotorTropicProofing##OTHER##,MotorThermistorFitted##OTHER##,MotorStarterSpeedControlType##OTHER##,MotorSize##ELECTRICAL_POWER##VOLT_AMPERES,MotorPoles##OTHER##,MotorManufacturer##OTHER##,MotorIngressProtectionRating##OTHER##,MotorFrame##OTHER##,MotorEfficiencyClass##OTHER##,MotorAmpsActual##ELECTRICAL_CURRENT##AMPERES,MotorAbsorbedPowerActual##ELECTRICAL_POWER##VOLT_AMPERES,MinorHubRadius##LENGTH##MILLIMETERS,MediumType##OTHER##,MediumDensity##HVAC_DENSITY##POUNDS_MASS_PER_CUBIC_FOOT,MajorHubRadius##LENGTH##MILLIMETERS,MaintenanceType##OTHER##,Location##OTHER##,LoadSubClassificationMotor##OTHER##,LoadClassification##OTHER##,Installer##OTHER##,InstallationDate##OTHER##,InletStaticPressureActual##HVAC_PRESSURE##PASCALS,InletPWL8kHz##OTHER##,InletPWL63Hz##OTHER##,InletPWL500Hz##OTHER##,InletPWL4kHz##OTHER##,InletPWL2kHz##OTHER##,InletPWL250Hz##OTHER##,InletPWL1kHz##OTHER##,InletPWL125Hz##OTHER##,InletConeInstalled##OTHER##,ImpellerBladePitch##ANGLE##DEGREES,ImpellerBladeMaterial##OTHER##,HazardClassification##OTHER##,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanType##OTHER##,FanStaticDutyPressure##HVAC_PRESSURE##PASCALS,FanStandard##OTHER##,FanRotationSpeedMax##OTHER##,FanRotationSpeedDesign##OTHER##,FanRotationSpeedActual##OTHER##,FanMEP##OTHER##,FanImpellerNoOfBlades##OTHER##,FanDiscInductPWL_Outlet##OTHER##,FanDiscInductPWL_Inlet##OTHER##,FanDesignArrangement##OTHER##,FanApplication##OTHER##,FanAirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowCalculated##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,ExpectedServiceLifeYears##OTHER##,EnergyMeterGrouping##OTHER##,Pressure Drop - Total##HVAC_PRESSURE##PASCALS,Pressure Drop - Static##HVAC_PRESSURE##PASCALS,Outlet Velocity##HVAC_VELOCITY##FEET_PER_MINUTE,Motor Input Power##ELECTRICAL_POWER##VOLT_AMPERES,Model##OTHER##,Manufacturer##OTHER##,Low Speed Start Current##ELECTRICAL_POWER##VOLT_AMPERES,Low Speed Full Load Current##ELECTRICAL_POWER##VOLT_AMPERES,E##LENGTH##MILLIMETERS,DynamicPressureActual##HVAC_PRESSURE##PASCALS,DuctSystemStaticPressureCalculated##HVAC_PRESSURE##PASCALS,DischargeStaticPressureActual##HVAC_PRESSURE##PASCALS,Designer##OTHER##,D##LENGTH##MILLIMETERS,ComponentStatus##OTHER##,ComponentName##OTHER##,CommissioningTechnician##OTHER##,CommissioningDate##OTHER##,Client##OTHER##,C##LENGTH##MILLIMETERS,BladeWidth##LENGTH##MILLIMETERS,BladeThickness##LENGTH##MILLIMETERS,BladeProjectionThickness##LENGTH##MILLIMETERS,BasisOfDesign##OTHER##,Barcode##OTHER##,B##ANGLE##DEGREES,AssetIdentifier##OTHER##,AirFlowMin##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowMax##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowCalc##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlow##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AbsorbedPower##ELECTRICAL_POWER##VOLT_AMPERES,Impeller Style##OTHER##,Impeller Limit Load Power##ELECTRICAL_POWER##VOLT_AMPERES,Impeller Absorbed  Power##ELECTRICAL_POWER##VOLT_AMPERES,Fan Material##OTHER##,Description##OTHER##,Default Elevation##LENGTH##MILLIMETERS,Approx Volume##VOLUME##CUBIC_METERS,Additional Notes##OTHER##,A##LENGTH##MILLIMETERS
HVLS30,0,,0,0,https://www.fantech.com.au,,0,0,,937.5,0,1,0,0,0,,0,25,100,,,,,,0,6,100,0,0,0,0,0,0,0,0,0,0,0,0,,1,,,,0,,,0,,,0,,0,0,,,,,0,0,150,,0,220,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,0,0,,,0,,0,,0,0,0,,,0,0,,,0,0,0,0,,0,0,0,0,HVLS30,Fantech,0,0,840,0,0,0,,1250,,,,,,350,120,6,15,,,5,,0,0,0,0,0,0,0,,0,0,Default,"The Gorilla range of high velocity, low speed (HVLS) fans generate a gentle, slow moving airstream that covers a large area even when they are installed in a very high ceiling",1219.2,0,,3050
HVLS40,0,,0,0,https://www.fantech.com.au,,0,0,,937.5,0,1,0,0,0,,0,25,100,,,,,,0,6,100,0,0,0,0,0,0,0,0,0,0,0,0,,1,,,,0,,,0,,,0,,0,0,,,,,0,0,150,,0,220,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,0,0,,,0,,0,,0,0,0,,,0,0,,,0,0,0,0,,0,0,0,0,HVLS40,Fantech,0,0,840,0,0,0,,1250,,,,,,450,120,6,15,,,5,,0,0,0,0,0,0,0,,0,0,Default,"The Gorilla range of high velocity, low speed (HVLS) fans generate a gentle, slow moving airstream that covers a large area even when they are installed in a very high ceiling",1219.2,0,,4050
HVLS40S,0,,0,0,https://www.fantech.com.au,,0,0,,952.5,0,1,0,0,0,,0,25,100,,,,,,0,6,100,0,0,0,0,0,0,0,0,0,0,0,0,,1,,,,0,,,0,,,0,,0,0,,,,,0,0,150,,0,220,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,0,0,,,0,,0,,0,0,0,,,0,0,,,0,0,0,0,,0,0,0,0,HVLS40S,Fantech,0,0,840,0,0,0,,1270,,,,,,450,120,6,15,,,5,,0,0,0,0,0,0,0,,0,0,Default,"The Gorilla range of high velocity, low speed (HVLS) fans generate a gentle, slow moving airstream that covers a large area even when they are installed in a very high ceiling",1219.2,0,,4050
HVLS50,0,,0,0,https://www.fantech.com.au,,0,0,,952.5,0,1,0,0,0,,0,25,100,,,,,,0,6,100,0,0,0,0,0,0,0,0,0,0,0,0,,1,,,,0,,,0,,,0,,0,0,,,,,0,0,150,,0,220,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,0,0,,,0,,0,,0,0,0,,,0,0,,,0,0,0,0,,0,0,0,0,HVLS50,Fantech,0,0,840,0,0,0,,1270,,,,,,550,120,6,15,,,5,,0,0,0,0,0,0,0,,0,0,Default,"The Gorilla range of high velocity, low speed (HVLS) fans generate a gentle, slow moving airstream that covers a large area even when they are installed in a very high ceiling",1219.2,0,,5050
HVLS60,0,,0,0,https://www.fantech.com.au,,0,0,,963,0,1,0,0,0,,0,25,100,,,,,,0,6,100,0,0,0,0,0,0,0,0,0,0,0,0,,1,,,,0,,,0,,,0,,0,0,,,,,0,0,150,,0,220,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,0,0,,,0,,0,,0,0,0,,,0,0,,,0,0,0,0,,0,0,0,0,HVLS60,Fantech,0,0,840,0,0,0,,1284,,,,,,550,120,6,15,,,5,,0,0,0,0,0,0,0,,0,0,Default,"The Gorilla range of high velocity, low speed (HVLS) fans generate a gentle, slow moving airstream that covers a large area even when they are installed in a very high ceiling",1219.2,0,,6050
HVLS60S,0,,0,0,https://www.fantech.com.au,,0,0,,978,0,1,0,0,0,,0,25,100,,,,,,0,6,100,0,0,0,0,0,0,0,0,0,0,0,0,,1,,,,0,,,0,,,0,,0,0,,,,,0,0,150,,0,220,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,0,0,,,0,,0,,0,0,0,,,0,0,,,0,0,0,0,,0,0,0,0,HVLS60S,Fantech,0,0,840,0,0,0,,1304,,,,,,550,120,6,15,,,5,,0,0,0,0,0,0,0,,0,0,Default,"The Gorilla range of high velocity, low speed (HVLS) fans generate a gentle, slow moving airstream that covers a large area even when they are installed in a very high ceiling",1219.2,0,,6050
HVLS70,0,,0,0,https://www.fantech.com.au,,0,0,,978,0,1,0,0,0,,0,25,100,,,,,,0,6,100,0,0,0,0,0,0,0,0,0,0,0,0,,1,,,,0,,,0,,,0,,0,0,,,,,0,0,150,,0,220,,,1,HVAC,,,0,0,0,0,0,0,0,0,0,0,0,,,0,,0,,0,0,0,,,0,0,,,0,0,0,0,,0,0,0,0,HVLS70,Fantech,0,0,840,0,0,0,,1304,,,,,,550,120,6,15,,,5,,0,0,0,0,0,0,0,,0,0,Default,"The Gorilla range of high velocity, low speed (HVLS) fans generate a gentle, slow moving airstream that covers a large area even when they are installed in a very high ceiling",1219.2,0,,7050
