,dB(A) @ 3m##OTHER##,ZoneServed##OTHER##,WireGuardInstalled##OTHER##,WarrantyDurationMonths##OTHER##,URL##OTHER##,TotalMass##MASS##KILOGRAMS,TotalEfficiency##HVAC_FACTOR##PERCENTAGE,SystemServed##OTHER##,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyPhase##OTHER##,SupplyFrequency##ELECTRICAL_FREQUENCY##HERTZ,SpringStaticDeflectionMin##LENGTH##MILLIMETERS,SoundPressureat3m##OTHER##,SerialNumber##OTHER##,RunLoadAmps##ELECTRICAL_CURRENT##AMPERES,Rev##LENGTH##MILLIMETERS,RFID##OTHER##,ProductCode##OTHER##,Pressure Drop - Total##HVAC_PRESSURE##PASCALS,Pressure Drop - Static##HVAC_PRESSURE##PASCALS,PrecommissioningInspectionTestPlan##OTHER##,PowerSource##OTHER##,PowerFactorState##OTHER##,PowerFactor##OTHER##,PeakPower##ELECTRICAL_POWER##WATTS,OverloadSettingActual##ELECTRICAL_CURRENT##AMPERES,OutletPWL8kHz##OTHER##,OutletPWL63Hz##OTHER##,OutletPWL500Hz##OTHER##,OutletPWL4kHz##OTHER##,OutletPWL2kHz##OTHER##,OutletPWL250Hz##OTHER##,OutletPWL1kHz##OTHER##,OutletPWL125Hz##OTHER##,OutletConeFitted##OTHER##,Outlet Velocity##HVAC_VELOCITY##METERS_PER_SECOND,OperatingTempMax##HVAC_TEMPERATURE##CELSIUS,OperatingMaintenanceManual##OTHER##,NCC_SEC_J_Compliance##OTHER##,NCC_Classification##OTHER##,NATspecWorkSection##OTHER##,MountingType##OTHER##,MountingFeetInstalled##OTHER##,MountingArrangement##OTHER##,MotorWindingInsulation##OTHER##,MotorVoltageActual##ELECTRICAL_POTENTIAL##VOLTS,MotorType##OTHER##,MotorTropicProofing##OTHER##,MotorThermistorFitted##OTHER##,MotorStarterSpeedControlType##OTHER##,MotorSize##ELECTRICAL_POWER##WATTS,MotorPoles##OTHER##,MotorManufacturer##OTHER##,MotorIngressProtectionRating##OTHER##,MotorFrame##OTHER##,MotorEfficiencyClass##OTHER##,MotorAmpsActual##ELECTRICAL_CURRENT##AMPERES,MotorAbsorbedPowerActual##ELECTRICAL_POWER##WATTS,Motor Input Power##ELECTRICAL_POWER##WATTS,Model##OTHER##,MediumType##OTHER##,MediumDensity##HVAC_DENSITY##KILOGRAMS_PER_CUBIC_METER,Manufacturer##OTHER##,MaintenanceType##OTHER##,Low Speed Start Current##ELECTRICAL_POWER##WATTS,Low Speed Full Load Current##ELECTRICAL_POWER##WATTS,Location##OTHER##,LoadSubClassificationMotor##OTHER##,LoadClassification##OTHER##,Installer##OTHER##,InstallationDate##OTHER##,InletStaticPressureActual##HVAC_PRESSURE##PASCALS,InletPWL8kHz##OTHER##,InletPWL63Hz##OTHER##,InletPWL500Hz##OTHER##,InletPWL4kHz##OTHER##,InletPWL2kHz##OTHER##,InletPWL250Hz##OTHER##,InletPWL1kHz##OTHER##,InletPWL125Hz##OTHER##,InletConeInstalled##OTHER##,ImpellerBladePitch##ANGLE##DEGREES,ImpellerBladeMaterial##OTHER##,Impeller Style##OTHER##,Impeller Limit Load Power##ELECTRICAL_POWER##WATTS,Impeller Diameter##LENGTH##MILLIMETERS,Impeller Absorbed  Power##ELECTRICAL_POWER##WATTS,HazardClassification##OTHER##,H##LENGTH##MILLIMETERS,G##LENGTH##MILLIMETERS,F##LENGTH##MILLIMETERS,Material##OTHER##,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanType##OTHER##,FanStaticDutyPressure##HVAC_PRESSURE##PASCALS,FanStandard##OTHER##,FanRotationSpeedMax##OTHER##,FanRotationSpeedDesign##OTHER##,FanRotationSpeedActual##OTHER##,FanMEP##OTHER##,FanImpellerNoOfBlades##OTHER##,FanHubDiameter##LENGTH##MILLIMETERS,FanDiscInductPWL_Outlet##OTHER##,FanDiscInductPWL_Inlet##OTHER##,FanDesignArrangement##OTHER##,FanApplication##OTHER##,FanAirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowCalculated##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,ExpectedServiceLifeYears##OTHER##,EnergyMeterGrouping##OTHER##,E##LENGTH##MILLIMETERS,DynamicPressureActual##HVAC_PRESSURE##PASCALS,DuctSystemStaticPressureCalculated##HVAC_PRESSURE##PASCALS,DischargeStaticPressureActual##HVAC_PRESSURE##PASCALS,DimensionalTolerance##LENGTH##MILLIMETERS,Designer##OTHER##,Description##OTHER##,D##LENGTH##MILLIMETERS,ComponentStatus##OTHER##,ComponentName##OTHER##,CommissioningTechnician##OTHER##,CommissioningDate##OTHER##,Client##OTHER##,Calc_h##LENGTH##MILLIMETERS,C-F##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,BasisOfDesign##OTHER##,Barcode##OTHER##,B##LENGTH##MILLIMETERS,AssetIdentifier##OTHER##,ArcRadius##LENGTH##MILLIMETERS,Approx Volume##VOLUME##CUBIC_METERS,AirFlowMin##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowMax##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowCalc##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlow##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AbsorbedPower##ELECTRICAL_POWER##WATTS,A##LENGTH##MILLIMETERS
TD-250/100SIL,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silent.pdf,0,0,,0,1,0,0,0,,0,553.911215,,,0,0,,,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,TD800/200ECO,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,97,575,121,<By Category>,0,,0,,0,0,0,,,0,0,0,,,0,0,0,0,,250,0,0,0,0,,"The TD Silent Series of low-profile mixed-flow in-line fans incorporates a break-through in noise reduction resulting in units that operate very quietly. The low noise levels are achieved through the technically advanced design of the internal construction, which does not impede on the air flow performance of the fan.",223,,,,,,48.5,102,223,,,83,,0,0,0,0,0,0,0,0,0,100
TD-250/100SILT-4PL,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silent.pdf,0,0,,0,1,0,0,0,,0,553.911215,,,0,0,,,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,TD800/200ECO,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,97,575,121,<By Category>,0,,0,,0,0,0,,,0,0,0,,,0,0,0,0,,250,0,0,0,0,,"The TD Silent Series of low-profile mixed-flow in-line fans incorporates a break-through in noise reduction resulting in units that operate very quietly. The low noise levels are achieved through the technically advanced design of the internal construction, which does not impede on the air flow performance of the fan.",223,,,,,,48.5,102,223,,,83,,0,0,0,0,0,0,0,0,0,100
TD-350/125SIL,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silent.pdf,0,0,,0,1,0,0,0,,0,424.7,,,0,0,,,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,TD800/200ECO,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,123,462,121,<By Category>,0,,0,,0,0,0,,,0,0,0,,,0,0,0,0,,250,0,0,0,0,,"The TD Silent Series of low-profile mixed-flow in-line fans incorporates a break-through in noise reduction resulting in units that operate very quietly. The low noise levels are achieved through the technically advanced design of the internal construction, which does not impede on the air flow performance of the fan.",223,,,,,,61.5,102,223,,,83,,0,0,0,0,0,0,0,0,0,100
TD-350/125SILT-4PL,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silent.pdf,0,0,,0,1,0,0,0,,0,424.7,,,0,0,,,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,TD800/200ECO,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,123,462,121,<By Category>,0,,0,,0,0,0,,,0,0,0,,,0,0,0,0,,250,0,0,0,0,,"The TD Silent Series of low-profile mixed-flow in-line fans incorporates a break-through in noise reduction resulting in units that operate very quietly. The low noise levels are achieved through the technically advanced design of the internal construction, which does not impede on the air flow performance of the fan.",223,,,,,,61.5,102,223,,,83,,0,0,0,0,0,0,0,0,0,100
TD-500/150SIL,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silent.pdf,0,0,,0,1,0,0,0,,0,510.3,,,0,0,,,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,TD800/200ECO,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,147,484,134,<By Category>,0,,0,,0,0,0,,,0,0,0,,,0,0,0,0,,250,0,0,0,0,,"The TD Silent Series of low-profile mixed-flow in-line fans incorporates a break-through in noise reduction resulting in units that operate very quietly. The low noise levels are achieved through the technically advanced design of the internal construction, which does not impede on the air flow performance of the fan.",251,,,,,,73.5,111,245,,,96,,0,0,0,0,0,0,0,0,0,116
TD-500/150SILT-4PL,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silent.pdf,0,0,,0,1,0,0,0,,0,510.3,,,0,0,,,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,TD800/200ECO,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,147,484,134,<By Category>,0,,0,,0,0,0,,,0,0,0,,,0,0,0,0,,250,0,0,0,0,,"The TD Silent Series of low-profile mixed-flow in-line fans incorporates a break-through in noise reduction resulting in units that operate very quietly. The low noise levels are achieved through the technically advanced design of the internal construction, which does not impede on the air flow performance of the fan.",251,,,,,,73.5,111,245,,,96,,0,0,0,0,0,0,0,0,0,116
TD-800/200SIL,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silent.pdf,0,0,,0,1,0,0,0,,0,846.1,,,0,0,,,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,TD800/200ECO,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,198,568,164,<By Category>,0,,0,,0,0,0,,,0,0,0,,,0,0,0,0,,340,0,0,0,0,,"The TD Silent Series of low-profile mixed-flow in-line fans incorporates a break-through in noise reduction resulting in units that operate very quietly. The low noise levels are achieved through the technically advanced design of the internal construction, which does not impede on the air flow performance of the fan.",296,,,,,,99,132,296,,,129,,0,0,0,0,0,0,0,0,0,145
TD-800/200SILT-4PL,0,,1,0,https://www.fantech.com.au/images/PDF/Catalogue/silent.pdf,0,0,,0,1,0,0,0,,0,846.1,,,0,0,,,0,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,TD800/200ECO,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,198,568,164,<By Category>,0,,0,,0,0,0,,,0,0,0,,,0,0,0,0,,340,0,0,0,0,,"The TD Silent Series of low-profile mixed-flow in-line fans incorporates a break-through in noise reduction resulting in units that operate very quietly. The low noise levels are achieved through the technically advanced design of the internal construction, which does not impede on the air flow performance of the fan.",296,,,,,,99,132,296,,,129,,0,0,0,0,0,0,0,0,0,145
