,x2##LENGTH##MILLIMETERS,x1##LENGTH##MILLIMETERS,calc_FØ_100N##LENGTH##MILLIMETERS,calc_EØ_100N##LENGTH##MILLIMETERS,ZoneServed##OTHER##,WireGuardInstalled##OTHER##,WarrantyDurationMonths##OTHER##,URL##OTHER##,Type Comments##OTHER##,TotalMass##MASS##KILOGRAMS,TotalEfficiency##HVAC_FACTOR##PERCENTAGE,SystemServed##OTHER##,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyPhase##OTHER##,SupplyFrequency##ELECTRICAL_FREQUENCY##HERTZ,SpringStaticDeflectionMin##LENGTH##MILLIMETERS,SerialNumber##OTHER##,RunLoadAmps##ELECTRICAL_CURRENT##AMPERES,RFID##OTHER##,ProductCode##OTHER##,Pressure Drop - Total##HVAC_PRESSURE##PASCALS,Pressure Drop - Static##HVAC_PRESSURE##PASCALS,PrecommissioningInspectionTestPlan##OTHER##,PowerSource##OTHER##,PowerFactorState##OTHER##,PowerFactor##OTHER##,PeakPower##ELECTRICAL_POWER##WATTS,OverloadSettingActual##ELECTRICAL_CURRENT##AMPERES,OutletPWL8kHz##OTHER##,OutletPWL63Hz##OTHER##,OutletPWL500Hz##OTHER##,OutletPWL4kHz##OTHER##,OutletPWL2kHz##OTHER##,OutletPWL250Hz##OTHER##,OutletPWL1kHz##OTHER##,OutletPWL125Hz##OTHER##,OutletConeFitted##OTHER##,Outlet Velocity##HVAC_VELOCITY##METERS_PER_SECOND,OperatingTempMax##HVAC_TEMPERATURE##CELSIUS,OperatingMaintenanceManual##OTHER##,OA_WIDTH##LENGTH##MILLIMETERS,NOZZLE_OUTLINE_OFFSET##LENGTH##MILLIMETERS,NCC_SEC_J_Compliance##OTHER##,NCC_Classification##OTHER##,NATspecWorkSection##OTHER##,MountingType##OTHER##,MountingFeetInstalled##OTHER##,MountingArrangement##OTHER##,MotorWindingInsulation##OTHER##,MotorVoltageActual##ELECTRICAL_POTENTIAL##VOLTS,MotorType##OTHER##,MotorTropicProofing##OTHER##,MotorThermistorFitted##OTHER##,MotorStarterSpeedControlType##OTHER##,MotorSize##ELECTRICAL_POWER##WATTS,MotorPoles##OTHER##,MotorManufacturer##OTHER##,MotorIngressProtectionRating##OTHER##,MotorFrame##OTHER##,MotorEfficiencyClass##OTHER##,MotorAmpsActual##ELECTRICAL_CURRENT##AMPERES,MotorAbsorbedPowerActual##ELECTRICAL_POWER##WATTS,Motor Input Power##ELECTRICAL_POWER##WATTS,Model##OTHER##,MediumType##OTHER##,MediumDensity##HVAC_DENSITY##KILOGRAMS_PER_CUBIC_METER,Manufacturer##OTHER##,MaintenanceType##OTHER##,MOUNT_SURF_BODY_LENGTH##LENGTH##MILLIMETERS,MOUNT_BRKT_LENGTH##LENGTH##MILLIMETERS,Low Speed Start Current##ELECTRICAL_POWER##WATTS,Low Speed Full Load Current##ELECTRICAL_POWER##WATTS,Location##OTHER##,LoadSubClassificationMotor##OTHER##,LoadClassification##OTHER##,Installer##OTHER##,InstallationDate##OTHER##,InletStaticPressureActual##HVAC_PRESSURE##PASCALS,InletPWL8kHz##OTHER##,InletPWL63Hz##OTHER##,InletPWL500Hz##OTHER##,InletPWL4kHz##OTHER##,InletPWL2kHz##OTHER##,InletPWL250Hz##OTHER##,InletPWL1kHz##OTHER##,InletPWL125Hz##OTHER##,InletConeInstalled##OTHER##,ImpellerBladePitch##ANGLE##DEGREES,ImpellerBladeMaterial##OTHER##,Impeller Style##OTHER##,Impeller Limit Load Power##ELECTRICAL_POWER##WATTS,Impeller Diameter##LENGTH##MILLIMETERS,Impeller Absorbed  Power##ELECTRICAL_POWER##WATTS,H##LENGTH##MILLIMETERS,HazardClassification##OTHER##,I##LENGTH##MILLIMETERS,G##LENGTH##MILLIMETERS,F_100N##LENGTH##MILLIMETERS,FAN_OFFSET_Y##LENGTH##MILLIMETERS,FAN_OFFSET_X##LENGTH##MILLIMETERS,FAN_INT_R##LENGTH##MILLIMETERS,FAN_EXT_R##LENGTH##MILLIMETERS,E_50N##LENGTH##MILLIMETERS,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanType##OTHER##,FanStaticDutyPressure##HVAC_PRESSURE##PASCALS,FanStandard##OTHER##,FanRotationSpeedMax##OTHER##,FanRotationSpeedDesign##OTHER##,FanRotationSpeedActual##OTHER##,FanMEP##OTHER##,FanImpellerNoOfBlades##OTHER##,FanHubDiameter##LENGTH##MILLIMETERS,FanDiscInductPWL_Outlet##OTHER##,FanDiscInductPWL_Inlet##OTHER##,FanDesignArrangement##OTHER##,FanApplication##OTHER##,FanAirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowCalculated##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,F_50N##LENGTH##MILLIMETERS,ExpectedServiceLifeYears##OTHER##,EnergyMeterGrouping##OTHER##,E_100N##LENGTH##MILLIMETERS,DynamicPressureActual##HVAC_PRESSURE##PASCALS,DuctSystemStaticPressureCalculated##HVAC_PRESSURE##PASCALS,DischargeStaticPressureActual##HVAC_PRESSURE##PASCALS,DimensionalTolerance##LENGTH##MILLIMETERS,Designer##OTHER##,Description##OTHER##,D##LENGTH##MILLIMETERS,ComponentStatus##OTHER##,ComponentName##OTHER##,CommissioningTechnician##OTHER##,CommissioningDate##OTHER##,Client##OTHER##,C##LENGTH##MILLIMETERS,BasisOfDesign##OTHER##,Barcode##OTHER##,BRKT_OA_WIDTH##LENGTH##MILLIMETERS,BRKT_CL##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,AssetIdentifier##OTHER##,Approximate Volume##VOLUME##CUBIC_METERS,Approx Volume##VOLUME##CUBIC_METERS,AirFlowMin##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowMax##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowCalc##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlow##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AbsorbedPower##ELECTRICAL_POWER##WATTS,A##LENGTH##MILLIMETERS
JIU-CPC2-50N,271.000000000000,711.000000000000,6.000000000000,6.500000000000,,1,0,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,JetVent Mixed-Flow Induction Fan,71.000000000000,0.000000000000,,415.000000000000,3,50.000000000000,0.000000000000,,0.000000000000,,,0.000000000000,0.000000000000,,,,0,0.000000000000,0.000000000000,0,0,0,0,0,0,0,0,1,0.000000000000,-273.150000000000,,930.000000000000,0.000000000000,1,,,,1,,,0.000000000000,,,1,,0.000000000000,0,,,,,0.000000000000,0.000000000000,0.000000000000,JIU-CPMF-50N,,0.000000000000,Fantech,,711.000000000000,454.000000000000,0.000000000000,0.000000000000,,1,HVAC,,,0.000000000000,0,0,0,0,0,0,0,0,1,0.000000000000,,,0.000000000000,0.000000000000,0.000000000000,395.000000000000,,325.000000000000,866.000000000000,12.000000000000,51.000000000000,395.000000000000,275.000000000000,330.000000000000,25.000000000000,0.000000000000,,0.000000000000,,0,,0,,,0.000000000000,0,0,,,0.000000000000,0.000000000000,0.000000000000,13.000000000000,0,,13.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,,The JIU Series mixed-flow induction unit is designed to provide general car park ventilation requirements. This unit is available in one size and has a very low profile housing making it a suitable option for installation in car parks with low ceiling height and obstructive structural beams. The JIU mixed-flow unit provides a uni-directional airflow and is suitable for ambient operating temperatures.,75.000000000000,,,,,,790.000000000000,,,930.000000000000,483.000000000000,271.000000000000,,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,1265.000000000000
JIU-CPC2-100N,333.000000000000,1156.000000000000,6.000000000000,13.500000000000,,1,0,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,JetVent Mixed-Flow Induction Fan,71.000000000000,0.000000000000,,415.000000000000,3,50.000000000000,0.000000000000,,0.000000000000,,,0.000000000000,0.000000000000,,,,0,0.000000000000,0.000000000000,0,0,0,0,0,0,0,0,1,0.000000000000,-273.150000000000,,1297.000000000001,25.000000000004,1,,,,1,,,0.000000000000,,,1,,0.000000000000,0,,,,,0.000000000000,0.000000000000,0.000000000000,JIU-CPMF-50N,,0.000000000000,Fantech,,1156.000000000000,800.000000000000,0.000000000000,0.000000000000,,1,HVAC,,,0.000000000000,0,0,0,0,0,0,0,0,1,0.000000000000,,,0.000000000000,0.000000000000,0.000000000000,700.000000000000,,1000.000000000000,1203.000000000000,12.000000000000,165.000000000000,572.000000000000,312.000000000000,367.500000000000,10.000000000000,0.000000000000,,0.000000000000,,0,,0,,,0.000000000000,0,0,,,0.000000000000,0.000000000000,0.000000000000,10.000000000000,0,,27.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,,The JIU Series mixed-flow induction unit is designed to provide general car park ventilation requirements. This unit is available in one size and has a very low profile housing making it a suitable option for installation in car parks with low ceiling height and obstructive structural beams. The JIU mixed-flow unit provides a uni-directional airflow and is suitable for ambient operating temperatures.,69.000000000000,,,,,,1147.000000000000,,,1247.000000000000,708.000000000000,333.000000000000,,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,0.000000000000,1830.000000000000
