,Description##OTHER##,CLEARANCE_LENGTH##LENGTH##MILLIMETERS,CLEARANCE_WIDTH##LENGTH##MILLIMETERS,CLEARANCE_HEIGHT##LENGTH##MILLIMETERS,Type Comments##OTHER##,URL##OTHER##,ZoneServed##OTHER##,DUCT_2-FAN_WIDTH##LENGTH##MILLIMETERS,DUCT_2-FAN_LENGTH##LENGTH##MILLIMETERS,DUCT_1-FAN_WIDTH##LENGTH##MILLIMETERS,DUCT_1-FAN_LENGTH##LENGTH##MILLIMETERS,CONNECTOR_LOCATION_LENGTH##LENGTH##MILLIMETERS,WireGuardInstalled##OTHER##,WarrantyDurationMonths##OTHER##,TotalMass##MASS##KILOGRAMS,TotalEfficiency##HVAC_FACTOR##PERCENTAGE,SystemServed##OTHER##,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyPhase##OTHER##,SupplyFrequency##ELECTRICAL_FREQUENCY##HERTZ,SpringStaticDeflectionMin##LENGTH##MILLIMETERS,SerialNumber##OTHER##,RunLoadAmps##ELECTRICAL_CURRENT##AMPERES,RFID##OTHER##,CLEARANCE_OFFSET##LENGTH##MILLIMETERS,CAP_HEIGHT##LENGTH##MILLIMETERS,ProductCode##OTHER##,Pressure Drop - Total##HVAC_PRESSURE##PASCALS,Pressure Drop - Static##HVAC_PRESSURE##PASCALS,PrecommissioningInspectionTestPlan##OTHER##,PowerSource##OTHER##,PowerFactorState##OTHER##,PowerFactor##OTHER##,PeakPower##ELECTRICAL_POWER##WATTS,H##LENGTH##MILLIMETERS,G##LENGTH##MILLIMETERS,OverloadSettingActual##ELECTRICAL_CURRENT##AMPERES,OutletPWL8kHz##OTHER##,OutletPWL63Hz##OTHER##,OutletPWL500Hz##OTHER##,OutletPWL4kHz##OTHER##,OutletPWL2kHz##OTHER##,OutletPWL250Hz##OTHER##,OutletPWL1kHz##OTHER##,OutletPWL125Hz##OTHER##,OutletConeFitted##OTHER##,Outlet Velocity##HVAC_VELOCITY##METERS_PER_SECOND,OperatingTempMax##HVAC_TEMPERATURE##CELSIUS,OperatingMaintenanceManual##OTHER##,NCC_SEC_J_Compliance##OTHER##,NCC_Classification##OTHER##,NATspecWorkSection##OTHER##,F##LENGTH##MILLIMETERS,MountingType##OTHER##,MountingFeetInstalled##OTHER##,MountingArrangement##OTHER##,MotorWindingInsulation##OTHER##,MotorVoltageActual##ELECTRICAL_POTENTIAL##VOLTS,MotorType##OTHER##,MotorTropicProofing##OTHER##,MotorThermistorFitted##OTHER##,MotorStarterSpeedControlType##OTHER##,MotorSize##ELECTRICAL_POWER##WATTS,MotorPoles##OTHER##,MotorManufacturer##OTHER##,MotorIngressProtectionRating##OTHER##,MotorFrame##OTHER##,MotorEfficiencyClass##OTHER##,MotorAmpsActual##ELECTRICAL_CURRENT##AMPERES,MotorAbsorbedPowerActual##ELECTRICAL_POWER##WATTS,Motor Input Power##ELECTRICAL_POWER##WATTS,Model##OTHER##,MediumType##OTHER##,MediumDensity##HVAC_DENSITY##KILOGRAMS_PER_CUBIC_METER,Manufacturer##OTHER##,MaintenanceType##OTHER##,Low Speed Start Current##ELECTRICAL_POWER##WATTS,Low Speed Full Load Current##ELECTRICAL_POWER##WATTS,Location##OTHER##,LoadSubClassificationMotor##OTHER##,LoadClassification##OTHER##,WB_BASE_DIA##LENGTH##MILLIMETERS,CAP_DIA##LENGTH##MILLIMETERS,BASE_LENGTH##LENGTH##MILLIMETERS,REVIT_MOUNT_DIA##LENGTH##MILLIMETERS,Installer##OTHER##,InstallationDate##OTHER##,InletStaticPressureActual##HVAC_PRESSURE##PASCALS,InletPWL8kHz##OTHER##,InletPWL63Hz##OTHER##,InletPWL500Hz##OTHER##,InletPWL4kHz##OTHER##,InletPWL2kHz##OTHER##,InletPWL250Hz##OTHER##,InletPWL1kHz##OTHER##,InletPWL125Hz##OTHER##,InletConeInstalled##OTHER##,ImpellerBladePitch##ANGLE##DEGREES,ImpellerBladeMaterial##OTHER##,Impeller Style##OTHER##,Impeller Limit Load Power##ELECTRICAL_POWER##WATTS,Impeller Diameter##LENGTH##MILLIMETERS,Impeller Absorbed  Power##ELECTRICAL_POWER##WATTS,HazardClassification##OTHER##,J##LENGTH##MILLIMETERS,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanType##OTHER##,FanStaticDutyPressure##HVAC_PRESSURE##PASCALS,FanStandard##OTHER##,FanRotationSpeedMax##OTHER##,FanRotationSpeedDesign##OTHER##,FanRotationSpeedActual##OTHER##,FanMEP##OTHER##,FanImpellerNoOfBlades##OTHER##,FanHubDiameter##LENGTH##MILLIMETERS,FanDiscInductPWL_Outlet##OTHER##,FanDiscInductPWL_Inlet##OTHER##,FanDesignArrangement##OTHER##,FanApplication##OTHER##,FanAirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowCalculated##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,ExpectedServiceLifeYears##OTHER##,EnergyMeterGrouping##OTHER##,DynamicPressureActual##HVAC_PRESSURE##PASCALS,DuctSystemStaticPressureCalculated##HVAC_PRESSURE##PASCALS,DischargeStaticPressureActual##HVAC_PRESSURE##PASCALS,DimensionalTolerance##LENGTH##MILLIMETERS,Designer##OTHER##,ComponentStatus##OTHER##,ComponentName##OTHER##,CommissioningTechnician##OTHER##,CommissioningDate##OTHER##,Client##OTHER##,BasisOfDesign##OTHER##,Barcode##OTHER##,BASE_WIDTH##LENGTH##MILLIMETERS,AssetIdentifier##OTHER##,Approx Volume##VOLUME##CUBIC_METERS,AirFlowMin##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowMax##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowCalc##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlow##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AbsorbedPower##ELECTRICAL_POWER##WATTS
TGU031,Gamma Ultra TCD/E 315 Diameter single and 3 phase twin centrifugal roof fan. The Gamma Series of centrifugal room units is generally used in ducted systems for a wide range of exhaust applications.,1443,747,393,Gamma Ultra Series Twin Fan roof units,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,,380,1080,380,380,1240,1,0,0,0,,230,1,50,0,,0,,40,314,,0,0,,,,0.8,0,353,75,0,0,0,0,0,0,0,0,0,1,0,-273.15,,1,,,667,,1,,,0,,,1,,0,0,,,,,0,0,0,TCE252,,0,Fantech,,0,0,,1,HVAC,483,483,1200,100,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,696,1.18,,0,,0,45 RPS,0,,,0,0,0,,,0,0,0,0,,0,0,0,0,,,,,,,,,500,,0.27,0,0,0,0,0,0,190
TGU035,Gamma Ultra TCD/E 355 Diameter single and 3 phase twin centrifugal roof fan. The Gamma Series of centrifugal room units is generally used in ducted systems for a wide range of exhaust applications.,1443,747,396,Gamma Ultra Series Twin Fan roof units,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,,380,1080,380,380,1240,1,0,0,0,,230,1,50,0,,0,,40,312,,0,0,,,,0.8,0,356,75,0,0,0,0,0,0,0,0,0,1,0,-273.15,,1,,,667,,1,,,0,,,1,,0,0,,,,,0,0,0,TCE252,,0,Fantech,,0,0,,1,HVAC,483,483,1200,100,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,696,1.18,,0,,0,45 RPS,0,,,0,0,0,,,0,0,0,0,,0,0,0,0,,,,,,,,,500,,0.27,0,0,0,0,0,0,190
TGU040,Gamma Ultra TCD/E 400 Diameter single and 3 phase twin centrifugal roof fan. The Gamma Series of centrifugal room units is generally used in ducted systems for a wide range of exhaust applications.,1974,1008,499,Gamma Ultra Series Twin Fan roof units,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,,600,1580,600,600,1740,1,0,0,0,,230,1,50,0,,0,,40,410,,0,0,,,,0.8,0,459,75,0,0,0,0,0,0,0,0,0,1,0,-273.15,,1,,,928,,1,,,0,,,1,,0,0,,,,,0,0,0,TCE252,,0,Fantech,,0,0,,1,HVAC,716,710,1700,100,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,966,1.18,,0,,0,45 RPS,0,,,0,0,0,,,0,0,0,0,,0,0,0,0,,,,,,,,,720,,0.27,0,0,0,0,0,0,190
TGU045,Gamma Ultra TCD/E 450 Diameter single and 3 phase twin centrifugal roof fan. The Gamma Series of centrifugal room units is generally used in ducted systems for a wide range of exhaust applications.,1974,1008,499,Gamma Ultra Series Twin Fan roof units,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,,600,1580,600,600,1740,1,0,0,0,,230,1,50,0,,0,,40,380,,0,0,,,,0.8,0,459,75,0,0,0,0,0,0,0,0,0,1,0,-273.15,,1,,,928,,1,,,0,,,1,,0,0,,,,,0,0,0,TCE252,,0,Fantech,,0,0,,1,HVAC,716,710,1700,100,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,966,1.18,,0,,0,45 RPS,0,,,0,0,0,,,0,0,0,0,,0,0,0,0,,,,,,,,,720,,0.27,0,0,0,0,0,0,190
TGU050,Gamma Ultra TCD/E 500 Diameter single and 3 phase twin centrifugal roof fan. The Gamma Series of centrifugal room units is generally used in ducted systems for a wide range of exhaust applications.,1974,1008,499,Gamma Ultra Series Twin Fan roof units,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,,600,1580,600,600,1740,1,0,0,0,,230,1,50,0,,0,,40,400,,0,0,,,,0.8,0,459,75,0,0,0,0,0,0,0,0,0,1,0,-273.15,,1,,,928,,1,,,0,,,1,,0,0,,,,,0,0,0,TCE252,,0,Fantech,,0,0,,1,HVAC,716,710,1700,100,,,0,0,0,0,0,0,0,0,0,1,0,,,0,0,0,,966,1.18,,0,,0,45 RPS,0,,,0,0,0,,,0,0,0,0,,0,0,0,0,,,,,,,,,720,,0.27,0,0,0,0,0,0,190
