,dB(A) @ 3m##OTHER##,ZoneServed##OTHER##,WireGuardInstalled##OTHER##,WheelRadius##LENGTH##MILLIMETERS,WarrantyDurationMonths##OTHER##,URL##OTHER##,Type Comments##OTHER##,TotalMass##MASS##KILOGRAMS,TotalEfficiency##HVAC_FACTOR##PERCENTAGE,SystemServed##OTHER##,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyPhase##OTHER##,SupplyFrequency##ELECTRICAL_FREQUENCY##HERTZ,SquareChannelLength##LENGTH##MILLIMETERS,SpringStaticDeflectionMin##LENGTH##MILLIMETERS,SoundPressureat3m##OTHER##,SerialNumber##OTHER##,RunLoadAmps##ELECTRICAL_CURRENT##AMPERES,RFID##OTHER##,ProductCode##OTHER##,Pressure Drop - Total##HVAC_PRESSURE##PASCALS,Pressure Drop - Static##HVAC_PRESSURE##PASCALS,PrecommissioningInspectionTestPlan##OTHER##,PowerSource##OTHER##,PowerFactorState##OTHER##,PowerFactor##OTHER##,PeakPower##ELECTRICAL_POWER##WATTS,OverloadSettingActual##ELECTRICAL_CURRENT##AMPERES,OutletPWL8kHz##OTHER##,OutletPWL63Hz##OTHER##,OutletPWL500Hz##OTHER##,OutletPWL4kHz##OTHER##,OutletPWL2kHz##OTHER##,OutletPWL250Hz##OTHER##,OutletPWL1kHz##OTHER##,OutletPWL125Hz##OTHER##,OutletConeFitted##OTHER##,Outlet Velocity##HVAC_VELOCITY##METERS_PER_SECOND,OperatingTempMax##HVAC_TEMPERATURE##CELSIUS,OperatingMaintenanceManual##OTHER##,NCC_SEC_J_Compliance##OTHER##,NCC_Classification##OTHER##,NATspecWorkSection##OTHER##,MountingType##OTHER##,MountingFeetInstalled##OTHER##,MountingArrangement##OTHER##,MotorWindingInsulation##OTHER##,MotorVoltageActual##ELECTRICAL_POTENTIAL##VOLTS,MotorType##OTHER##,MotorTropicProofing##OTHER##,MotorThermistorFitted##OTHER##,MotorStarterSpeedControlType##OTHER##,MotorSize##ELECTRICAL_POWER##WATTS,MotorPoles##OTHER##,MotorManufacturer##OTHER##,MotorIngressProtectionRating##OTHER##,MotorFrame##OTHER##,MotorEfficiencyClass##OTHER##,MotorAmpsActual##ELECTRICAL_CURRENT##AMPERES,MotorAbsorbedPowerActual##ELECTRICAL_POWER##WATTS,Motor Input Power##ELECTRICAL_POWER##WATTS,Model##OTHER##,MediumType##OTHER##,MediumDensity##HVAC_DENSITY##KILOGRAMS_PER_CUBIC_METER,Manufacturer##OTHER##,MaintenanceType##OTHER##,Low Speed Start Current##ELECTRICAL_POWER##WATTS,Low Speed Full Load Current##ELECTRICAL_POWER##WATTS,Location##OTHER##,LoadSubClassificationMotor##OTHER##,LoadClassification##OTHER##,Installer##OTHER##,InstallationDate##OTHER##,InletStaticPressureActual##HVAC_PRESSURE##PASCALS,InletPWL8kHz##OTHER##,InletPWL63Hz##OTHER##,InletPWL500Hz##OTHER##,InletPWL4kHz##OTHER##,InletPWL2kHz##OTHER##,InletPWL250Hz##OTHER##,InletPWL1kHz##OTHER##,InletPWL125Hz##OTHER##,InletConeInstalled##OTHER##,ImpellerBladePitch##ANGLE##DEGREES,ImpellerBladeMaterial##OTHER##,HazardClassification##OTHER##,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FrameThicknessRadius##LENGTH##MILLIMETERS,FrameThickness##LENGTH##MILLIMETERS,FrameDepth##LENGTH##MILLIMETERS,FanType##OTHER##,FanStaticDutyPressure##HVAC_PRESSURE##PASCALS,FanStandard##OTHER##,FanRotationSpeedMax##OTHER##,FanRotationSpeedDesign##OTHER##,FanRotationSpeedActual##OTHER##,FanRadius##LENGTH##MILLIMETERS,FanMEP##OTHER##,FanImpellerNoOfBlades##OTHER##,FanHubDiameter##LENGTH##MILLIMETERS,FanDiscInductPWL_Outlet##OTHER##,FanDiscInductPWL_Inlet##OTHER##,FanDiamter##LENGTH##MILLIMETERS,FanDesignArrangement##OTHER##,FanApplication##OTHER##,FanAirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowCalculated##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,FanAirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,Impeller Style##OTHER##,Impeller Limit Load Power##ELECTRICAL_POWER##WATTS,Impeller Diameter##LENGTH##MILLIMETERS,Impeller Absorbed  Power##ELECTRICAL_POWER##WATTS,ExpectedServiceLifeYears##OTHER##,EnergyMeterGrouping##OTHER##,E##LENGTH##MILLIMETERS,DynamicPressureActual##HVAC_PRESSURE##PASCALS,DuctSystemStaticPressureCalculated##HVAC_PRESSURE##PASCALS,DischargeStaticPressureActual##HVAC_PRESSURE##PASCALS,DimensionalTolerance##LENGTH##MILLIMETERS,Designer##OTHER##,D##LENGTH##MILLIMETERS,ComponentStatus##OTHER##,ComponentName##OTHER##,CommissioningTechnician##OTHER##,CommissioningDate##OTHER##,Client##OTHER##,Description##OTHER##,CaseRadius##LENGTH##MILLIMETERS,CaseDiameter##LENGTH##MILLIMETERS,CaseDepth##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,BoxHeight##LENGTH##MILLIMETERS,BasisOfDesign##OTHER##,Barcode##OTHER##,B##LENGTH##MILLIMETERS,AssetIdentifier##OTHER##,Approx Volume##VOLUME##CUBIC_METERS,AirFlowMin##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowMax##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowDesign##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowCalc##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlowActual##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AirFlow##HVAC_AIR_FLOW##CUBIC_METERS_PER_SECOND,AbsorbedPower##ELECTRICAL_POWER##WATTS,A##LENGTH##MILLIMETERS
CCE404,0,,1,80,0,https://www.fantech.com.au/images/PDF/Catalogue/CompactCooler.pdf,New Generation Series,0,0,,0,1,0,20,0,0,,0,,,0,0,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,CCE404,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,227.5,5,30,,0,,0,0,0,252.5,,,0,0,0,505,,,0,0,0,,0,0,0,0,,150,0,0,0,0,,585,,,,,,The Alpha & Beta Industrial Series of axial roof units are designed for a wide range of free intake and ducted exhaust systems. These durable and robust units feature adjustable pitch impellers which allows for optimum air flow and power efficiency,222.5,445,220,745,257.5,,,615,,0,0,0,0,0,0,0,0,440
CCE564,0,,1,80,0,https://www.fantech.com.au/images/PDF/Catalogue/CompactCooler.pdf,New Generation Series,0,0,,0,1,0,20,0,0,,0,,,0,0,,,,0,0,0,0,0,0,0,0,0,0,0,1,0,0,,1,,,,1,,,0,,,1,,0,0,,,,,0,0,0,CCE564,,0,Fantech,,0,0,,1,HVAC,,,0,0,0,0,0,0,0,0,0,1,0,,,0,330,5,30,,0,,0,0,0,355,,,0,0,0,710,,,0,0,0,,0,0,0,0,,150,0,0,0,0,,640,,,,,,The Alpha & Beta Industrial Series of axial roof units are designed for a wide range of free intake and ducted exhaust systems. These durable and robust units feature adjustable pitch impellers which allows for optimum air flow and power efficiency,325,650,220,845,360,,,820,,0,0,0,0,0,0,0,0,540
