,A##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,URL##OTHER##,Model##OTHER##,Description##OTHER##,Revision##OTHER##
PCEEC31DD,400,433,500,https://www.fantech.com.au/FanRange.aspx?RangeID=2065&mountingID=,PCEEC31DD,"The ECOtronic EC Series of Powerline centrifugal fan incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control. It is suitable for supply or exhaust from applications ranging from residential through commercial to industrial, where medium to high air pressure is required",A
PCEEC35DD,450,483,550,https://www.fantech.com.au/FanRange.aspx?RangeID=2065&mountingID=,PCEEC35DD,"The ECOtronic EC Series of Powerline centrifugal fan incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control. It is suitable for supply or exhaust from applications ranging from residential through commercial to industrial, where medium to high air pressure is required",A
PCEEC40DD,500,533,550,https://www.fantech.com.au/FanRange.aspx?RangeID=2065&mountingID=,PCEEC40DD,"The ECOtronic EC Series of Powerline centrifugal fan incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control. It is suitable for supply or exhaust from applications ranging from residential through commercial to industrial, where medium to high air pressure is required",A
PCDEC45DD,550,583,600,https://www.fantech.com.au/FanRange.aspx?RangeID=2065&mountingID=,PCDEC45DD,"The ECOtronic EC Series of Powerline centrifugal fan incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control. It is suitable for supply or exhaust from applications ranging from residential through commercial to industrial, where medium to high air pressure is required",A
PCDEC50DD,650,683,700,https://www.fantech.com.au/FanRange.aspx?RangeID=2065&mountingID=,PCDEC50DD,"The ECOtronic EC Series of Powerline centrifugal fan incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control. It is suitable for supply or exhaust from applications ranging from residential through commercial to industrial, where medium to high air pressure is required",A
PCDEC56DD,725,758,800,https://www.fantech.com.au/FanRange.aspx?RangeID=2065&mountingID=,PCDEC56DD,"The ECOtronic EC Series of Powerline centrifugal fan incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control. It is suitable for supply or exhaust from applications ranging from residential through commercial to industrial, where medium to high air pressure is required",A
