,y1##LENGTH##MILLIMETERS,x1##LENGTH##MILLIMETERS,calc_g##LENGTH##MILLIMETERS,calc_d##LENGTH##MILLIMETERS,calc_c##LENGTH##MILLIMETERS,URL##OTHER##,TotalMass##MASS##KILOGRAMS,SupplyVoltage##ELECTRICAL_POTENTIAL##VOLTS,SupplyPhase##OTHER##,SupplyFrequency##ELECTRICAL_FREQUENCY##HERTZ,Model##OTHER##,GØ##LENGTH##MILLIMETERS,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,FanRotationSpeedDesign##OTHER##,F##LENGTH##MILLIMETERS,E##LENGTH##MILLIMETERS,DØ##LENGTH##MILLIMETERS,Description##OTHER##,CØ##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,Approx Volume##VOLUME##CUBIC_METERS,AbsorbedPower##ELECTRICAL_POWER##WATTS,A##LENGTH##MILLIMETERS
HXM-200,86,266,4.5,105.5,102.5,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,0,0,1,0,HXM-200,9,0,0,19,86,211,"The HXM Series of wall mounted square plate fans is designed for general ventilation applications such as cafes, bars, commercial premises and small workshops etc.  This range is recommended for mounting on a wall or vertical partition only. Refer to the Ring Plate Series or Compact 2000 Series for ceiling/horizontal applications.",205,222,0,0,266
HXM-250,93,333,4.5,130.5,127.5,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,0,0,1,0,HXM-250,9,0,0,31,93,261,"The HXM Series of wall mounted square plate fans is designed for general ventilation applications such as cafes, bars, commercial premises and small workshops etc.  This range is recommended for mounting on a wall or vertical partition only. Refer to the Ring Plate Series or Compact 2000 Series for ceiling/horizontal applications.",255,276,0,0,333
HXM-300,93,400,5.25,155.5,152.5,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,0,0,1,0,HXM-300,10.5,0,0,36,93,311,"The HXM Series of wall mounted square plate fans is designed for general ventilation applications such as cafes, bars, commercial premises and small workshops etc.  This range is recommended for mounting on a wall or vertical partition only. Refer to the Ring Plate Series or Compact 2000 Series for ceiling/horizontal applications.",305,337,0,0,400
HXM-350,106,465,5.25,185.5,180.5,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,0,0,1,0,HXM-350,10.5,0,0,35,106,371,"The HXM Series of wall mounted square plate fans is designed for general ventilation applications such as cafes, bars, commercial premises and small workshops etc.  This range is recommended for mounting on a wall or vertical partition only. Refer to the Ring Plate Series or Compact 2000 Series for ceiling/horizontal applications.",361,390,0,0,465
HXM-400,141,500,5,207,200,http://www.fantech.com.au/update/fanselupdate.asp?pv=4.050603&dv=4.10,0,0,1,0,HXM-400,10,0,0,52,141,414,"The HXM Series of wall mounted square plate fans is designed for general ventilation applications such as cafes, bars, commercial premises and small workshops etc.  This range is recommended for mounting on a wall or vertical partition only. Refer to the Ring Plate Series or Compact 2000 Series for ceiling/horizontal applications.",400,420,0,0,500
