,Description##OTHER##,A##LENGTH##MILLIMETERS,B1##LENGTH##MILLIMETERS,B2##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,D##LENGTH##MILLIMETERS,E##LENGTH##MILLIMETERS,F##LENGTH##MILLIMETERS,G##LENGTH##MILLIMETERS,H##LENGTH##MILLIMETERS,I##LENGTH##MILLIMETERS,TotalMass##MASS##KILOGRAMS,Model##OTHER##,I1##LENGTH##MILLIMETERS,FullLoadAmps##ELECTRICAL_CURRENT##AMPERES,AbsorbedPower##ELECTRICAL_POWER##WATTS,Revision##OTHER##
JETLINE-100,Jetline Series - Mixed-Flow Fans,276,15,15,181,95,256,306,70,98,70,3,JETLINE-100,0,0.1,19,A
JETLINE-125,Jetline Series - Mixed-Flow Fans,279,15,15,206,120,265,315,70,111,70,3.4,JETLINE-125,0,0.2,40,A
JETLINE-150,Jetline Series - Mixed-Flow Fans,323,20,20,243.5,145,298.5,348,70,130,70,4.5,JETLINE-150,0,0.4,83,A
JETLINE-200,Jetline Series - Mixed-Flow Fans,322,30,30,273,195,320,369,100,144.5,70,5.6,JETLINE-200,0,0.5,125,A
JETLINE-250,Jetline Series - Mixed-Flow Fans,329,20,30,293,245,326,375,120,154.3,50,6.5,JETLINE-250,25,0.7,160,A
JETLINE-315,Jetline Series - Mixed-Flow Fans,369,20,33,322,310,357.5,407,120,170,50,8.9,JETLINE-315,25,0.9,215,A
JETLINE-100ECO,Jetline Ecowatt Series - Mixed-Flow Fans,276,15,15,181,95,256,306,70,98,70,2.5,JETLINE-100ECO,0,0.1,16,A
JETLINE-125ECO,Jetline Ecowatt Series - Mixed-Flow Fans,279,15,15,206,120,265,315,70,111,70,2.8,JETLINE-125ECO,0,0.2,26,A
JETLINE-150ECO,Jetline Ecowatt Series - Mixed-Flow Fans,323,20,20,243.5,145,298.5,348,70,130,70,3.6,JETLINE-150ECO,0,0.5,58,A
JETLINE-200ECO,Jetline Ecowatt Series - Mixed-Flow Fans,322,30,30,273,195,320,369,100,144.5,70,4.7,JETLINE-200ECO,0,0.8,109,A
JETLINE-250ECO,Jetline Ecowatt Series - Mixed-Flow Fans,329,20,30,293,245,326,375,120,154.3,50,5.8,JETLINE-250ECO,25,0.9,135,A
JETLINE-315ECO,Jetline Ecowatt Series - Mixed-Flow Fans,369,20,33,322,310,357.5,407,120,170,50,8,JETLINE-315ECO,25,0.13,194,A
