,A##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,D##LENGTH##MILLIMETERS,E##LENGTH##MILLIMETERS,F##LENGTH##MILLIMETERS,G##LENGTH##MILLIMETERS,H##LENGTH##MILLIMETERS,J##LENGTH##MILLIMETERS,Description##OTHER##,URL##OTHER##,Model##OTHER##,TotalMass##MASS##KILOGRAMS,Revision##OTHER##
RIL-100,100,60,115,80,303,97,180,205,215,The ProVent Series of in-line mixed-flow fans have been specifically designed for ducted supply or exhaust air applications,https://www.fantech.com.au/FanRange.aspx?RangeID=223&mountingID=,RIL-100,2,B
RIL-125,100,60,115,80,258,123,180,205,215,The ProVent Series of in-line mixed-flow fans have been specifically designed for ducted supply or exhaust air applications,https://www.fantech.com.au/FanRange.aspx?RangeID=223&mountingID=,RIL-125,2,B
RIL-150SW,112,60,127,80,295,147,203,225,239,The ProVent Series of in-line mixed-flow fans have been specifically designed for ducted supply or exhaust air applications,https://www.fantech.com.au/FanRange.aspx?RangeID=223&mountingID=,RIL-150SW,2.7,B
RIL-150TSW,112,60,127,80,295,147,203,225,239,The ProVent Series of in-line mixed-flow fans have been specifically designed for ducted supply or exhaust air applications,https://www.fantech.com.au/FanRange.aspx?RangeID=223&mountingID=,RIL-150TSW,2.7,B
RIL-200SW,124,94,141,100,302,198,220,251,265,The ProVent Series of in-line mixed-flow fans have been specifically designed for ducted supply or exhaust air applications,https://www.fantech.com.au/FanRange.aspx?RangeID=223&mountingID=,RIL-200SW,4.9,B
RIL-200TSW,124,94,141,100,302,198,220,251,265,The ProVent Series of in-line mixed-flow fans have been specifically designed for ducted supply or exhaust air applications,https://www.fantech.com.au/FanRange.aspx?RangeID=223&mountingID=,RIL-200TSW,4.9,B
