,AØ##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,DØ##LENGTH##MILLIMETERS,EØ##LENGTH##MILLIMETERS,Description##OTHER##,URL##OTHER##,Model##OTHER##,TotalMass##MASS##KILOGRAMS,Tile Roof Flashing##OTHER##,Metal deck flashing##OTHER##,Revision##OTHER##
ECE152T,140,100,700,285,150,The Ezifit Thru Roof exhaust fan is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECE152T,4,1,0,B
ECE152M,140,100,700,285,150,The Ezifit Thru Roof exhaust fan is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECE152M,4,0,1,B
ECE154T,140,100,700,285,150,The Ezifit Thru Roof exhaust fan is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECE154T,4,1,0,B
ECE154M,140,100,700,285,150,The Ezifit Thru Roof exhaust fan is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECE154M,4,0,1,B
ECE204T,194,153,752,445,200,The Ezifit Thru Roof exhaust fan is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECE204T,10.5,1,0,B
ECE204M,194,153,752,445,200,The Ezifit Thru Roof exhaust fan is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECE204M,10.5,0,1,B
ECEP152T,139,133,745,290,150,The Ezifit Thru Roof exhaust fan with plastic top cap is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECEP152T,5,1,0,A
ECEP152M,139,133,745,290,150,The Ezifit Thru Roof exhaust fan with plastic top cap is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECEP152M,5,0,1,A
ECEP154T,139,133,745,290,150,The Ezifit Thru Roof exhaust fan with plastic top cap is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECEP154T,5,1,0,A
ECEP154M,139,133,745,290,150,The Ezifit Thru Roof exhaust fan with plastic top cap is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECEP154M,5,0,1,A
ECEP156T,139,133,745,290,150,The Ezifit Thru Roof exhaust fan with plastic top cap is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECEP156T,5,1,0,A
ECEP156M,139,133,745,290,150,The Ezifit Thru Roof exhaust fan with plastic top cap is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECEP156M,5,0,1,A
ECEP204T,195,194,790,443,200,The Ezifit Thru Roof exhaust fan with plastic top cap is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECEP204T,10,1,0,A
ECEP204M,195,194,790,443,200,The Ezifit Thru Roof exhaust fan with plastic top cap is easy to install and provides high air flow with a low noise output.,https://www.fantech.com.au/FanRange.aspx?AppID=D4&RangeID=165,ECEP204M,10,0,1,A
