,A##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,URL##OTHER##,Model##OTHER##,Description##OTHER##,Revision##OTHER##
PCEEC28A,350,383,350,https://www.fantech.com.au/FanRange.aspx?RangeID=207&mountingID=,PCEEC28A,"The PowerLineŽ EC Series of In-Line centrifugal fans incorporate the latest state-of-the-art, energy saving EC motor technology and are most efficient where conditions vary during the course of the day.",A
PCEEC31A,400,433,400,https://www.fantech.com.au/FanRange.aspx?RangeID=207&mountingID=,PCEEC31A,"The PowerLineŽ EC Series of In-Line centrifugal fans incorporate the latest state-of-the-art, energy saving EC motor technology and are most efficient where conditions vary during the course of the day.",A
PCEEC35A,450,483,425,https://www.fantech.com.au/FanRange.aspx?RangeID=207&mountingID=,PCEEC35A,"The PowerLineŽ EC Series of In-Line centrifugal fans incorporate the latest state-of-the-art, energy saving EC motor technology and are most efficient where conditions vary during the course of the day.",A
PCDEC40A,500,533,450,https://www.fantech.com.au/FanRange.aspx?RangeID=207&mountingID=,PCEEC40A,"The PowerLineŽ EC Series of In-Line centrifugal fans incorporate the latest state-of-the-art, energy saving EC motor technology and are most efficient where conditions vary during the course of the day.",A
PCDEC45A,550,583,475,https://www.fantech.com.au/FanRange.aspx?RangeID=207&mountingID=,PCDEC45A,"The PowerLineŽ EC Series of In-Line centrifugal fans incorporate the latest state-of-the-art, energy saving EC motor technology and are most efficient where conditions vary during the course of the day.",A
