,A##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,D##LENGTH##MILLIMETERS,E##LENGTH##MILLIMETERS,Description##OTHER##,URL##OTHER##,Model##OTHER##,TotalMass##MASS##KILOGRAMS,Revision##OTHER##
MRV1,210,260,55,200,310,Alpha Relief Air Vents have been designed for air intake and exhaust applications or control of pressure within buildings.,https://www.fantech.com.au/FanData.aspx?&RangeID=41,MRV1,1,B
MRV2,350,410,55,350,570,Alpha Relief Air Vents have been designed for air intake and exhaust applications or control of pressure within buildings.,https://www.fantech.com.au/FanData.aspx?&RangeID=41,MRV2,3,B
RV1,400,500,95,380,670,Alpha Relief Air Vents have been designed for air intake and exhaust applications or control of pressure within buildings.,https://www.fantech.com.au/FanData.aspx?&RangeID=41,RV1,5,B
RV2,510,610,90,450,770,Alpha Relief Air Vents have been designed for air intake and exhaust applications or control of pressure within buildings.,https://www.fantech.com.au/FanData.aspx?&RangeID=41,RV2,7,B
RV3,670,770,90,560,890,Alpha Relief Air Vents have been designed for air intake and exhaust applications or control of pressure within buildings.,https://www.fantech.com.au/FanData.aspx?&RangeID=41,RV3,11,B
RV4,780,980,85,640,1180,Alpha Relief Air Vents have been designed for air intake and exhaust applications or control of pressure within buildings.,https://www.fantech.com.au/FanData.aspx?&RangeID=41,RV4,16,B
RV5,900,1100,85,700,1395,Alpha Relief Air Vents have been designed for air intake and exhaust applications or control of pressure within buildings.,https://www.fantech.com.au/FanData.aspx?&RangeID=41,RV5,20,B
RV6,1100,1360,85,630,1640,Alpha Relief Air Vents have been designed for air intake and exhaust applications or control of pressure within buildings.,https://www.fantech.com.au/FanData.aspx?&RangeID=41,RV6,23,B