,A##LENGTH##MILLIMETERS,B##LENGTH##MILLIMETERS,C##LENGTH##MILLIMETERS,D##LENGTH##MILLIMETERS,E##LENGTH##MILLIMETERS,F##LENGTH##MILLIMETERS,G##LENGTH##MILLIMETERS,H##LENGTH##MILLIMETERS,J##LENGTH##MILLIMETERS,Description##OTHER##,URL##OTHER##,Model##OTHER##,TotalMass##MASS##KILOGRAMS,NCC_SEC_J_Compliance##OTHER##,Revision##OTHER##
CPEEC25DD,250,261,275,370,320,197,74,15,7,The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control,https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC25DD,10,0,A
CPEEC31DD,315,326,360,430,380,201,85,15,10,The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control,https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC31DD,11,0,A
CPEEC35DD,350,361,395,485,435,194,85,15,10,The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control,https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC35DD,11,1,A
CPEEC40DD,400,411,450,540,490,178,95,15,10,The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control,https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC40DD,13,1,A
CPEEC45DD,450,461,500,575,535,206,95,15,10,The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control,https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC45DD,15,0,A
CPEEC50DD,500,512,560,655,615,250,100,15,10,The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control,https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC50DD,21,0,A
CPEEC56DD,560,577,620,725,670,251,100,15,10,The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control,https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC56DD,24,0,A
CPEEC63DD,630,647,700,805,750,256,105,20,10,The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control,https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC63DD,27,1,A
CPEEC71DD,710,725,765,850,810,240,125,20,14.5,The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control,https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC71DD,29,0,A
CPEEC25DDR,250,261,275,370,320,197,74,15,7,"Reverse Flow, The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control",https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC25DDR,10,1,A
CPEEC31DDR,315,326,360,430,380,201,85,15,10,"Reverse Flow, The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control",https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC31DDR,11,1,A
CPEEC35DDR,350,361,395,485,435,194,85,15,10,"Reverse Flow, The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control",https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC35DDR,11,1,A
CPEEC40DDR,400,411,450,540,490,178,95,15,10,"Reverse Flow, The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control",https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC40DDR,13,1,A
CPEEC45DDR,450,461,500,575,535,206,95,15,10,"Reverse Flow, The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control",https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC45DDR,15,1,A
CPEEC50DDR,500,512,560,655,615,250,100,15,10,"Reverse Flow, The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control",https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC50DDR,21,0,A
CPEEC56DDR,560,577,620,725,670,251,100,15,10,"Reverse Flow, The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control",https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC56DDR,24,0,A
CPEEC63DDR,630,647,700,805,750,256,105,20,10,"Reverse Flow, The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control",https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC63DDR,27,0,A
CPEEC71DDR,710,725,765,850,810,240,125,20,14.5,"Reverse Flow, The ECOtronic EC Series of square plate axial fans incorporates an IE5* rated Electronically Commutated (EC) shaft motor delivering ultra energy efficient operation with the benefit of in-built variable speed control",https://www.fantech.com.au/FanRange.aspx?RangeID=2052&mountingID=,CPEEC71DDR,29,0,A
